**LAST SHOT  
WARNING BELL**

**ANTI-CHEAT  
RELAY**

**K29-1400 COIL**

**GAME OVER  
RELAY**

**L28-500 COIL**

**USE THREE  
1½ VOLT  
FLASH LIGHT  
BATTERIES**

**SERVICE  
OUTLET**

**PUCK SHOT  
RELAY**

**D28-1200 COIL**

8

6

4

2

3 AMP.  
110 VOLT

5 AMP.  
30 VOLT

3 AMP.  
6 VOLT

**BATTERY  
JACK**

**ON**

**OFF**

**N O T I C E**

**Battery Jack Is Used For  
Shipping Purposes Only To  
Disconnect Anti-Cheat Bell  
In Transit. Jack Should  
Be In "ON" Position At All  
Other Times.**

FRAME

ADJ JACK

**C A U T I O N**

**RED INDICATES 110 VOLTS**

**FRAME & COUNT  
UNIT**

**Finger Ass'y.  
No. 243-2501  
CONTACT PLATE  
No. 243-2501**

**Rev.**

**"B-1" SWITCH**

**Steps Up Frame  
Unit.**

**"B-2" SWITCH**

**Rings Last Shot  
Warning Bell.**

**"C" SWITCH**

**Runs Motor.**

**PUCK COUNT  
MOTOR UNIT**

**NO. 1227 MOTOR  
24 R.P.M.**

**"A" SWITCH**

**Energizes Shot  
Relay.**

Fonts used: FangSong, Bebas Neue

The lower 4 labels should be stickers.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.