ASSEMBLY INSTRUCTIONS

FEED REQUIRED AMOUNT OF LINE CORD THRU SLOT IN PEDESTAL. MOUNT THE  
LIGHTBOX ON TOP OF PEDESTAL WITH MACHINE SCREWS AND WASHERS PROVIDED.

REMOVE THE SHIPPING SCREW HOLDING PLUG MOUNTING PANEL.

INSTALL PLUGS IN SOCKETS ON PANEL.

HANG PANEL WITH PLUG AND SOCKETS INTO PEDESTAL HOLE. THIS WILL ALLOW  
THE LIGHTBOX INSERT TO BE LOWERED FOR SERVICING.

A-9487-1

222

ASSEMBLY INSTRUCTIONS

FEED REQUIRED AMOUNT OF LINE CORD THRU SLOT IN PEDESTAL. MOUNT THE  
LIGHTBOX ON TOP OF PEDESTAL WITH MACHINE SCREWS AND WASHERS PROVIDED.

REMOVE THE SHIPPING SCREW HOLDING PLUG MOUNTING PANEL.

INSTALL PLUGS IN SOCKETS ON PANEL.

HANG PANEL WITH PLUG AND SOCKETS INTO PEDESTAL HOLE. THIS WILL ALLOW  
THE LIGHTBOX INSERT TO BE LOWERED FOR SERVICING.

A-9487-1

222

Used fonts: Futura Md BT

Card size: 102x76mm.

**Cards status:**

A-9487-1 Assembly Instructions card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work ,please send me a donation via PayPal.