– RESET SW.

– EXTRA CHUTE COUNT SW.

INSIDE SW. – EXTRA CHUTE COUNT

SECOND SW. – TARGET SCORING

THIRD SW. – BANK RESET


FOURTH SW. – MATCH

FIFTH SW. – ADD TARGET UNITS

MOTOR 4A

MOTOR 4B

MOTOR SWITCH POSITIONS



MOTOR 4C

#

3½

INSIDE SW. – TARGET SCORING.

SECOND SW. – MATCH

#

4

MOTOR 3B

#

3

INSIDE SW. – RESET EXTRA CHUTE,  
 ADD BALLS PLAYED

SECOND SW. – SCORING

– TARGET SCORING SW.

INSIDE SW. – MOTOR RUNOUT

SECOND SW. – OPENS CIRCUIT TO  
 PLAYBOARD CONTACTS.

THIRD SW. – OPENS CIRCUIT TO  
 TARGET LIGHTS.

FOURTH SW. – OPENS CIRCUIT TO  
 REPLAY BUTTON

– ADD BALLS PLAYED SW.

MOTOR 1A

#

2

INSIDE SW. “W” RELAY LOCKIN

SECOND SW. – “B” RELAY LOCKIN

THIRD SW. – TARGET RELAY LOCKIN

INSIDE SW. – TARGET SCORING

SECOND SW. – SECOND PLAYER  
 RELAY

THIRD SW. – TOTAL PLAY METER,  
 SUBTRACT REPLAY


FOURTH SW. – IN LINE STEPOFF

MOTOR 1B

MOTOR 2B

#

1



MOTOR 1C

MOTOR 2C

E

D

C

B

A

MOTOR 1D

157

SK414-20

Font used: Futura Hv BT, Futura Md BT, News Gothic Demi

Size:102x203mm

**Cards status:**

Sk414-20 Motor Switch Positions card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.