# BANK-A-BALL

## HITTING NUMBERS 1 TO 7 OR 9 TO 15 LIGHTS EIGHT BALL. HITTING EIGHT BALL LIGHTS A ROLLOVER FOR SPECIAL. NUMBERS SCORE 5 POINTS WHEN OUT OR AS INDICATED. SPECIAL WHEN LIT TARGET AND ROLLOVER SCORE 1 REPLAY.

## MATCHING LAST NUMBER IN POINT SCORE TO LIGHTED NUMBER THAT APPEARS ON BACK GLASS WHEN GAME IS OVER AWARDS 1 REPLAY.

217

A-9033

# BANK-A-BALL

## HITTING NUMBERS 1 TO 7 OR 9 TO 15 LIGHTS EIGHT BALL. HITTING EIGHT BALL LIGHTS A ROLLOVER FOR SPECIAL. NUMBERS SCORE 5 POINTS WHEN OUT OR AS INDICATED. SPECIAL WHEN LIT TARGET AND ROLLOVER SCORE 1 REPLAY.

217

A-9034

1 REPLAY FOR 900 POINTS.

1 REPLAY FOR 1100 POINTS.

1 REPLAY FOR 1200 POINTS.

1 REPLAY FOR 1300 POINTS.

1 REPLAY FOR 1200 POINTS.

1 REPLAY FOR 1400 POINTS.

1 REPLAY FOR 1600 POINTS.

1 REPLAY FOR 1800 POINTS.

1 REPLAY FOR 1200 POINTS.

1 REPLAY FOR 1600 POINTS.

1 REPLAY FOR 1700 POINTS.

1 REPLAY FOR 1800 POINTS.

A-9038

1 REPLAY FOR 1100 POINTS.

1 REPLAY FOR 1300 POINTS.

1 REPLAY FOR 1500 POINTS.

1 REPLAY FOR 1700 POINTS.

1 REPLAY FOR 1100 POINTS.

1 REPLAY FOR 1400 POINTS.

1 REPLAY FOR 1500 POINTS.

1 REPLAY FOR 1600 POINTS.

A-8492

BANK SET-UP

CAUTION

REPLACE ONLY WITH

1 -AMP. SLO-BLO FUSE

A-5522

HAVE YOU CLEANED  
THE PLAYFIELD?

HAVE YOU REPLACED  
BURNED OUT BULBS?

A-6505

TOTAL PLAY

M E T E R

A-4702

3-5 BALL  
ADJUSTMENT

A-7747

3

5

**POINT SCORE ADJUSTMENT**

**1500 - 500 1000**

**1400 - 400 900 - 1900**

**1300 - 300 800 - 1800**

**1200 - 200 700 - 1700**

**1100 - 100 600 - 1600**

PLUG IN BLUE  
WIRE FOR  
SCORES 100  
TO 1000.

PLUG IN RED  
WIRE FOR SCORES 1100  
TO 1900.

**A-6521**

THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED  
TRANSFORMER TO MAINTAIN THE USUAL FINE FLIP-  
PER ACTION AT LOW VOLTAGE. MOVING THE RED  
WITH YELLOW TRACER WIRE ON THE TRANSFORMER  
FROM THE NORMAL TAP TO THE HIGH TAP ALLOWS  
THE MACHINE TO OPERATE AT A REDUCED VOLTAGE.  
IN NO CASE SHOULD THE RED WITH YELLOW TRACER  
WIRE BE LEFT ON THE HIGH TAP WHEN THE LOCA-  
TION VOLTAGE EQUALS OR EXCEEDS 110 VOLTS.

A-6279

V

50 POINT  
RELAY

O

MATCH  
RELAY

P

SERIES  
RELAY

R

115V  
HOLD  
RELAY

U

5 POINT  
RELAY

C

SCORE  
DELAY  
RELAY

W

EXTRA  
CHUTE  
RELAY

Strip size: 368x25mm. Stitch the relay labels after V and the blank before U

1 TO 7

SEQUENCE  
RELAY

A-1118  
COIL

9 TO 15

SEQUENCE  
RELAY

A-1118  
COIL

8A

EIGHT BALL  
REPLAY RELAY

A-1118  
COIL

H

THOUSAND  
RELAY

A-1118  
COIL

D

RESET  
RELAY

A-1118  
COIL

X

GAME OVER  
RELAY

A-1118  
COIL

SS

START  
RELAY

A-7112  
COIL

S

BANK RESET  
RELAY

A-1118  
COIL

T

TILT  
RELAY

A-1118  
COIL

Strip size: 274x17mm

Used fonts: Futura Md BT, Futura Bk BT

Card size: 154x108mm (instructions and score cards)

**Cards status:**

A-9033 instruction card confirmed.

A-9034 instruction card confirmed.

A-8492 score card confirmed.

A-9038 score card confirmed.

Relay strips confirmed.

**Cards available in separate files:**

A-9487-1 Assembly Instructions,

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.