# BUCCANEER

# INSTRUCTIONS

**3 BALLS PER PLAY**

## HITTING 2 OR 3 GIVES 2 AND 3. HITTING 6 OR 7 GIVES 6 AND 7. HITTING 8 OR 9 GIVES 8 AND 9.

## COMPLETING 1 THROUGH 11 SEQUENCE LIGHTS CENTER ROLLOVERS ALTERNATELY FOR SPECIAL.

## BLUE POP BUMPERS SCORE 100 POINTS OR 1000 WHEN LIT.

## YELLOW BUMPERS SCORE 1000 POINTS.

## SPIN TARGET SCORES 100 POINTS AND IF LIT SPOTS INDICATED NUMBER.

## SPECIAL SCORES ONE REPLAY.

MATCHING LAST TWO NUMBERS IN SCORE TO NUMBER THAT APPEARS  
 ON BACK GLASS AFTER GAME IS OVER SCORES ONE REPLAY.

390

B-16416-1

# BUCCANEER

# INSTRUCTIONS

**5 BALLS PER PLAY**

## COMPLETING 1 THROUGH 11 SEQUENCE LIGHTS CENTER ROLLOVERS ALTERNATELY FOR SPECIAL.

## BLUE POP BUMPERS SCORE 10 POINTS OR 100 WHEN LIT.

## YELLOW BUMPERS SCORE 100 POINTS.

## SPIN TARGET SCORES 100 POINTS AND IF LIT SPOTS INDICATED NUMBER.

## SPECIAL SCORES ONE REPLAY.

MATCHING LAST TWO NUMBERS IN SCORE TO NUMBER THAT APPEARS  
 ON BACK GLASS AFTER GAME IS OVER SCORES ONE REPLAY.

390

B-16416-1

ADJUSTMENT PLUG LOCATION

BOTTOM PANEL 1st COIN CHUTE, 2nd CHUTE

ADJ., TILT RESET ADJ. AND

SPIN “N” SPOT ADJ. (LIB. POS.)

LIGHTBOX HIGH SCORE ADJ.

PLAYBOARD 3-5 BALL ADJ.

**SCORE CARDS ARE LISTED FROM LIBERAL TO  
CONSERVATIVE. RECOMMENDED CARD  
IS MARKED †.**

**NOTE: DUE TO ELECTRICAL ADJUSTMENTS  
THE 3 BALL SCORES ARE THE SAME  
AS THE 5 BALL SCORES.**

A-16800 100,000 - 150,000

A-16419 110,000 - 130,000 - 160,000

A-16420 110,000 - 150,000 - 170,000

† A-16421 110,000 - 140,000

A-16422 110,000 - 150,000

A-16423 110,000 - 160,000

A-16424 120,000 - 140,000

A-16425 120,000 - 150,000

A-16426 120,000 - 160,000

A-16427 120,000 - 170,000

A-16428 130,000 - 150,000

A-16429 130,000 - 160,000

A-16430 130,000 - 170,000

A-16431 140,000 - 180,000

A-16418-2

390



1 REPLAY FOR EACH SCORE OF 100,000 POINTS.

1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

A-16800

1 REPLAY FOR EACH SCORE OF 110,000 POINTS.

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.

1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-16419

1 REPLAY FOR EACH SCORE OF 110,000 POINTS.

1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

1 REPLAY FOR EACH SCORE OF 170,000 POINTS.

A-16420

1 REPLAY FOR EACH SCORE OF 110,000 POINTS.

1 REPLAY FOR EACH SCORE OF 140,000 POINTS.

A-16421

1 REPLAY FOR EACH SCORE OF 110,000 POINTS.

1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

A-16422

1 REPLAY FOR EACH SCORE OF 110,000 POINTS.

1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-16423

1 REPLAY FOR EACH SCORE OF 120,000 POINTS.

1 REPLAY FOR EACH SCORE OF 140,000 POINTS.

A-16424

1 REPLAY FOR EACH SCORE OF 120,000 POINTS.

1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

A-16425

1 REPLAY FOR EACH SCORE OF 120,000 POINTS.

1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-16426

1 REPLAY FOR EACH SCORE OF 120,000 POINTS.

1 REPLAY FOR EACH SCORE OF 170,000 POINTS.

A-16427

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.

1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

A-16428

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.

1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-16429

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.

1 REPLAY FOR EACH SCORE OF 170,000 POINTS.

A-16430

1 REPLAY FOR EACH SCORE OF 140,000 POINTS.

1 REPLAY FOR EACH SCORE OF 180,000 POINTS.

A-16431

1 REPLAY FOR EACH SCORE OF POINTS.  
1 REPLAY FOR EACH SCORE OF POINTS.  
1 REPLAY FOR EACH SCORE OF POINTS.

A-12689-1

1 REPLAY FOR EACH SCORE OF POINTS.  
1 REPLAY FOR EACH SCORE OF POINTS.

A-16141

SPIN “N” SPOT

ADJUSTMENT

A-16432

CON. LIB.

25

VOLT

FUSE

**10**

AMP.

PLAYBOARD

LIGHT

FUSE

**10**

AMP.

LIGHTBOX

LIGHT

FUSE

**7½**

AMP.

LINE VOLTAGE

2 COINS 3 PLAYS  
RELAY

PRIMARY FUSE  
5 AMP. SLO-BLO

**1ST COIN CHUTE**

**ADJUSTMENT**

**2ND 1 COIN**

**CHUTE 1 PLAY**

**A-16081**

**TILT** **RESET**

**ADJUSTMENT**

**IN**

**OUT**

A-9609

**2ND COIN CHUTE**

**ADJUSTMENT**

**2 COINS  
3 PLAYS**

**1 COIN**

**A-16080**

**2ND CHUTE RELAY  
ADJUSTMENT**

**A-16082**

**5 PLAYS**

**4 PLAYS**

**3 PLAYS**

**2 PLAYS**

**1 PLAY**

D

500  
POINT  
RELAY

O

BALL  
RETURN  
RELAY

E

5000  
POINT  
RELAY

W

2nd  
CHUTE  
RELAY

F

ADVANCE  
UNIT  
SPOTTING  
RELAY

S

START  
RELAY

H

TILT  
HOLD  
RELAY

P

SPIN  
TARGET  
RELAY

R

HOLD  
RELAY

G

SPIN  
TARGET  
DELAY  
RELAY

T

TILT  
RELAY

Q

SERIES  
RELAY

Fonts used: Futura BdCn BT, Futura Hv BT, Futura Bk BT, Futura XBlk BT, News Gothic Std.

Card size: 108x154mm (instruction cards), 57x154mm (score cards).

**Cards status:**

B-16416-1 instruction cards confirmed.

A-16418-2 score index card confirmed.

All score cards confirmed.

All labels confirmed.

Relay strip confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.