**COIN CHUTE CHANGEOVER**

WHEN CHANGING THIS GAME FROM A SINGLE CHUTE  
MODEL TO A DOUBLE CHUTE MODEL REMOVE PLUG COV-  
ERING REJECT ROD HOLE.

REMOVE BAFFLE PLATE BLOCKING RIGHT HAND POR-  
TION OF COIN RETURN TROUGH. REPLACE COIN EN-  
TRANCE PLATE AND ASSEMBLE ALL COIN CHUTE PARTS  
SIMILAR TO LEFT HAND CHUTE. REWIRE GAME WITH NEW  
DOOR CABLE AND “W” RELAY. USE “W” RELAY WIRING  
DIAGRAM AND GAME SCHEMATIC CIRCUIT FOR PROPER  
CONNECTIONS.

A-7497

Fonts used: Futura Md BT

**Cards status:**

A-7497 card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.