
MOTOR SWITCH POSITIONS

MOTOR 3½ B - BRAKE



#2

#3

#3½

INSIDE SW. – “S”, “W” & “XX” RELAY LOCKINS.

MOTOR 2B SECOND SW. – “C” & “U” RELAY LOCKINS.

THIRD SW. – ACTUATES “D” RELAY.

INSIDE SW. – COIN CHUTE CREDIT TOTALIZER.

SECOND SW. – SUBTRACT REPLAY, ADD TOTAL  
MOTOR 2C PLAY METER.

(L-POSITION) THIRD SW. – ADDS REPLAY ON MATCH.

FOURTH SW. – RESETS SEQUENCE BANK.

FIFTH SW. – ACTUATES #1 TO #10 SEQUENCE  
 RELAYS.

MOTOR 4B INSIDE SW. – COIN CHUTE CREDIT TOTALIZER.

SECOND SW. – ACTUATES BALL RETURN KICKER.

INSIDE SW. – COIN CHUTE CREDIT TOTALIZER.

MOTOR 4C SECOND SW. – “0” RELAY LOCKIN.

(S-POSITION) THIRD SW. – RESETS CONTROL BANK.

#1

INSIDE SW. – RESETS SCORE UNITS.

MOTOR 1A SECOND SW. – SCORING.

(S-POSITION) THIRD SW. – COMPLETES CIRCUIT TO  
 “X” RELAY.


INSIDE SW. – MOTOR RUNOUT.

SECOND SW. – OPENS CIRCUIT TO  
MOTOR 1C PLAYBOARD CONTACTS.

(S-POSITION) THIRD SW. – COMPLETES CIRCUIT TO  
 REPLAY BUTTON.

FOURTH SW. – COMPLETES CIRCUIT TO  
 #11 RELAY.

#4



C

B


A

S L

256 C-11300

MOTOR SWITCH POSITIONS

MOTOR 3½ B - BRAKE



INSIDE SW. – “S”, “W” & “XX” RELAY LOCKINS.

MOTOR 2B SECOND SW. – “C” & “U” RELAY LOCKINS.

THIRD SW. – ACTUATES “D” RELAY.

INSIDE SW. – SUBTRACT REPLAY, ADD TOTAL PLAY METER.

MOTOR 2C SECOND SW. – ADDS REPLAY ON MATCH.

(L-POSITION) THIRD SW. – RESETS SEQUENCE BANK.

FOURTH SW. – ACTUATES #1 TO #10 SEQUENCE  
 RELAYS.

#2

#3

#3½

MOTOR 4B SW. – ACTUATES BALL RETURN KICKER.

MOTOR 4C INSIDE SW. – “0” RELAY LOCKIN.

(S-POSITION) SECOND SW. – RESETS CONTROL BANK.

#1

INSIDE SW. – RESETS SCORE UNITS.

MOTOR 1A SECOND SW. – SCORING.

(S-POSITION) THIRD SW. – COMPLETES CIRCUIT TO  
 “X” RELAY.


INSIDE SW. – MOTOR RUNOUT.

SECOND SW. – OPENS CIRCUIT TO  
MOTOR 1C PLAYBOARD CONTACTS.

(S-POSITION) THIRD SW. – COMPLETES CIRCUIT TO  
 REPLAY BUTTON.

FOURTH SW. – COMPLETES CIRCUIT TO  
 #11 RELAY.

#4



C

B

A

S L

256 C-11300

Font used:

Size:102x203mm

**Cards status:**

C-11300 Motor Switch Position black card confirmed.

C-11300 Motor Switch Position red card (without coin chute credit totalizers) confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.