
MOTOR SWITCH POSITIONS



#

MOTOR 4A SW. – RESET.

(S-Position)

INSIDE SW. – EXTRA CHUTE COUNT.

MOTOR 4B SECOND SW. – ADD BALLS PLAYED.

INSIDE SW. – EXTRA CHUTE COUNT.  
 SECOND SW. – OPENS CIRCUIT TO  
MOTOR 4C 0-9 ADD COIL.

(S-Position) THIRD SW. – SCORING.

FOURTH SW. – BANK RESET.

3½

MOTOR 3½ B - BRAKE

4

#

INSIDE SW. – ROTO UNIT SCORING.

MOTOR 3B SECOND SW. – SCORE 2ND PLAYER  
 MATCH.

MOTOR 3E SW. – ROTO ANTI-CYCLE.

#

3

INSIDE SW. – RESET EXTRA CHUTE  
MOTOR 1A COUNT, ADD BALLS PLAYED.

(S-Position) SECOND SW. – SCORING.

THIRD SW. – ROTO UNIT SCORING.

MOTOR 1B INSIDE SW. – ROTO UNIT SCORING.  
 SECOND SW. – TRIPS "QB" RELAY.

INSIDE SW. – MOTOR RUNOUT.

SECOND SW. – OPENS CIRCUIT TO " XB"  
 RELAY.

MOTOR 1C THIRD SW. – OPENS REPLAY BUTTON  
(S-Position) CIRCUIT.

FOURTH SW. – OPENS CIRCUIT TO "F"  
 RELAY.

MOTOR 1D SW. – ROTO UNIT SCORING.

INSIDE SW. – OPENS CIRCUIT TO

"BB" & "G" LOCKINS.

SECOND SW. – OPENS CIRCUIT TO

MOTOR 2B "F", "I", "J" & "X"  
 LOCKINS

THIRD SW. – OPENS CIRCUIT TO "E"  
 "K" & "W" LOCKINS.

INSIDE SW. – ROTO UNIT SCORING.

SECOND SW. – EXTRA CHUTE COUNT.


MOTOR 2C THIRD SW. – SUBTRACT REPLAYS,   
(L-Position) TOTAL PLAY METER. FOURTH SW. – SCORES 1ST PLAYER  
 MATCH.  
 FIFTH SW. – ADD BALLS PLAYED.

2

#

1

#



E

D

C

B

A

*S L*

216 B-8988-2

Font used: Futura Hv BT, Futura Md BT

Size:102x203mm

**Cards status:**

B-8988-2 Motor Switch Positions card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.