## TO REPLACE LIGHT BULBS DEPRESS CATCH AT TOP OF CABINET AND SWING INSERT DOWN.

## VERY IMPORTANT

## BE SURE TO INSERT ALL LIGHT BOX PLUGS BEFORE ATTACHING CORD TO 110V. LINE. DO NOT MAKE ANY ADJUSTMENTS ON CONTACTS OR STEP SWITCHES WHILE MACHINE IS CONNECTED TO 110V. LINE.

## SK130

## TO REPLACE LIGHT BULBS DEPRESS CATCH AT TOP OF CABINET AND SWING INSERT DOWN.

## VERY IMPORTANT

## BE SURE TO INSERT ALL LIGHT BOX PLUGS BEFORE ATTACHING CORD TO 110V. LINE. DO NOT MAKE ANY ADJUSTMENTS ON CONTACTS OR STEP SWITCHES WHILE MACHINE IS CONNECTED TO 110V. LINE.

## SK130

**Cards status:**

Used fonts: Futura Md BT, Futura Hv BT

SK130 Very Important card confirmed. (102x128mm).

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.