**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**PLAYFIELD ILLUMINATION  
7-1/2 AMP NORMAL–BLO  
32V**

**LIGHTBOX ILLUMINATION  
15 AMP NORMAL–BLO  
32V**

**SOLENOIDS  
8 AMP SLO–BLO  
250V**

**CONTROLLED LAMPS & SWITCHES  
10 AMP SLO–BLO  
32V**

**POWER SUPPLY (A2)  
2-1/2 AMP SLO–BLO  
250V**

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**WARNING – FOR CONTINUED PROTECTION AGAINST FIRE  
HAZARD, REPLACE ONLY WITH A FUSE OF THE SAME TYPE  
AND HAVING THE SAME ELECTRICAL RATING.**

**ATTENTION: UTILISER UN FUSIBLE DE RECHANGE  
 DE MEME TYPE DE …A …V.**

**31945**

F3

F11

F10

F9

F8

F7

F6

F5

F4

**31556**

F3

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**PLAYFIELD ILLUMINATION  
7-1/2 AMP NORMAL–BLO  
32V**

**LIGHTBOX ILLUMINATION  
15 AMP NORMAL–BLO  
32V**

**SOLENOIDS  
8 AMP SLO–BLO  
250V**

**CONTROLLED LAMPS & SWITCHES  
10 AMP SLO–BLO  
32V**

**POWER SUPPLY (A2)  
2-1/2 AMP SLO–BLO  
250V**

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**WARNING – FOR CONTINUED PROTECTION AGAINST FIRE  
HAZARD, REPLACE ONLY WITH A FUSE OF THE SAME TYPE  
AND HAVING THE SAME ELECTRICAL RATING.**

**ATTENTION: UTILISER UN FUSIBLE DE RECHANGE  
 DE MEME TYPE DE …A …V.**

F11

F10

F9

F8

F7

F6

F5

F4

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**PLAYFIELD ILLUMINATION  
10 AMP SLO–BLO  
32V**

**LIGHTBOX ILLUMINATION  
15 AMP NORMAL–BLO  
32V**

**SOLENOIDS  
8 AMP SLO–BLO  
250V**

**CONTROLLED LAMPS & SWITCHES  
10 AMP SLO–BLO  
32V**

**POWER SUPPLY (A2)  
2-1/2 AMP SLO–BLO  
250V**

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**WARNING – FOR CONTINUED PROTECTION AGAINST FIRE HAZARD, REPLACE ONLY  
WITH A FUSE OF THE SAME TYPE AND  
HAVING THE SAME ELECTRICAL RATING.**

**ATTENTION: UTILISER UN FUSIBLE DE RECHANGE DE MEME TYPE DE …A …V.**

**29522**

F3

F11

F10

F9

F8

F7

F6

F5

F4

**PRIMARY POWER  
5 AMP SLO-BLO/110V AC  
2.5 AMP SLO-BLO/220V AC**

F2

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**AUX. POWER SUPPLY (A5)  
3 AMP SLO–BLO  
250V**

**PLAYFIELD ILLUMINATION  
15 AMP NORMAL–BLO  
32V**

**LIGHTBOX ILLUMINATION  
15 AMP NORMAL–BLO  
32V**

**SOLENOIDS  
8 AMP SLO–BLO  
250V**

**CONTROLLED LAMPS & SWITCHES  
10 AMP SLO–BLO  
32V**

**POWER SUPPLY (A2)  
2-1/2 AMP SLO–BLO  
250V**

**DISPLAY  
3/8 AMP SLO–BLO  
250V**

**WARNING – FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD, REPLACE ONLY  
WITH A FUSE OF THE SAME TYPE AND  
HAVING THE SAME ELECTRICAL RATING.**

F3

**30094**

F11

F10

F9

F8

F7

F6

F5

F4

Fonts used: News Gothic Std.

Card size 80x148mm

**Cards status:**

29522 (Cueball Wizard) fuse card confirmed.

31556 (Big Hurt) fuse card confirmed.

31945 (Strikes N Spares) fuse card confirmed.

30094 (Gladiators) fuse card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.