**WARNING — FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A  
FUSE OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

**DISPLAY FILAMENT**

**1 AMP NORMAL-BLO**

**32 V**

**PLAYFIELD ILLUMINATION**

**5 AMP SLO-BLO**

**250 V**

**CONTROLLED LAMPS**

**8 AMP SLO-BLO**

**250 V**

**SOLENOIDS (+24V DC)**

**8 AMP SLO-BLO**

**250 V**

**DISPLAY (32V AC)**

**0.25 AMP SLO-BLO**

**250 V**

**POWER SUPPLY (A2)**

**6.25 AMP SLO-BLO**

**250 V**

**SOUND POWER SUPPLY (A5)**

**0.50 AMP NORMAL-BLO**

**32 V**

**F9**

**F9A**

**F6**

**F5**

**F4**

**F3**

**F2**

**F1**

**F8**

**PRIMARY POWER**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**LIGHTBOX ILLUMINATION**

**0.50 AMP**

**250V. SLO-BLO**

**F7**

**A-25470**

**WARNING — FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A  
FUSE OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

**PLAYFIELD ILLUMINATION**

**5 AMP**

**250V. SLO–BLO**

**CONTROLLED LAMPS**

**10 AMP**

**250V. SLO–BLO**

**SOLENOIDS (+24V DC)**

**8 AMP**

**250V. SLO–BLO**

**DISPLAY (32V AC)**

**0.25 AMP**

**250V. SLO–BLO**

**POWER SUPPLY (A2)**

**6.25 AMP**

**250 V. SLO–BLO**

**SOUND POWER SUPPLY (A5)**

**0.50 AMP**

**250V. NORMAL–BLO**

**A-25029**

**F7**

**F6**

**F5**

**F4**

**F3**

**F2**

**F1**

**F8**

**LIGHTBOX ILLUMINATION**

**0.50 AMP**

**250V. SLO-BLO**

**PRIMARY POWER**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**WARNING — FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A  
FUSE OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

**SOUND SPEECH (WHEN USED)**

**LIGHTBOX ILLUMINATION**

**10 AMP.**

**250V. SLO–BLO**

**PLAYFIELD ILLUMINATION**

**8 AMP.**

**250V. SLO–BLO**

**CONTROLLED LAMPS**

**10 AMP.**

**250V. SLO–BLO**

**SOLENOIDS (+24V DC)**

**8 AMP.**

**250V. SLO–BLO**

**DISPLAY (60V AC)**

**0.25 AMP.**

**250V. SLO–BLO**

**POWER SUPPLY (A2)**

**5 AMP.**

**250 V. SLO–BLO**

**SOUND POWER SUPPLY (A6)**

**0.50 AMP.**

**250V. NORMAL–BLO**

**PRIMARY POWER**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**F6**

**F8**

**A-24421**

**F1**

**F5**

**F3**

**F2**

**F4**

**F7**

**F15**

**WARNING — FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A  
FUSE OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

**10 AMP**

**250V. SLO–BLO**

**8 AMP**

**250V. SLO–BLO**

**7.5 AMP**

**250V. SLO–BLO**

**8 AMP**

**250V. SLO–BLO**

**0.25 AMP**

**250V. SLO–BLO**

**5 AMP**

**250 V. SLO–BLO**

**0.50 AMP.**

**250V. NORMAL–BLO**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**F8**

**F7**

**F6**

**F5**

**F4**

**F3**

**F2**

**F1**

**A-25096**

**WARNING — FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A FUSE  
OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

**PLAYFIELD ILLUMINATION**

**6.25 AMP**

**250V. SLO–BLO**

**CONTROLLED LAMPS**

**8 AMP**

**250V. SLO–BLO**

**SOLENOIDS (+24V DC)**

**8 AMP**

**250V. SLO–BLO**

**DISPLAY (32V AC)**

**0.25 AMP**

**250V. SLO–BLO**

**POWER SUPPLY (A2)**

**6.25 AMP**

**250 V. SLO–BLO**

**SOUND POWER SUPPLY (A5)**

**0.50 AMP**

**250V. NORMAL–BLO**

**F6**

**F7**

**F8**

**F1**

**F5**

**F3**

**F2**

**F4**

**LIGHTBOX ILLUMINATION**

**0.50 AMP**

**250V. SLO-BLO**

**PRIMARY POWER**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**ATTENTION — POUR ASSURER LA PROTECTION  
CONTRE LES SURTENSIONS NE REMPLACER LES FUSI-  
BLES QUE PAR DES FUSIBLES D’ORIGINE AYANT LES  
MEMES CARACTERISTIQUES ELECTRIQUE.**

**FILAMENT DE L’AFFICHEUR  
1 AMP NORMAL BLO  
250V**

**ILLUMINATION DU PLATEAU  
5 AMP SLO–BLO  
250V**

**LAMPES CONTROLLEES  
8 AMP SLO–BLO  
250V**

**BOBINES  
8 AMP SLO–BLO  
250V**

**AFFICHEURS  
0.25 AMP SLO–BLO  
250V**

**ALIMENTATION  
6.25 AMP SLO–BLO  
250V**

**ALIMENTATION PLAQUE SON  
0.50 AMP NORMAL–BLO  
250V**

**F8**

**FUSIBLE PRIMAIRE**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**ILLUMINATION DU FRONTON**

**.50 AMP SLO-BLO**

**250 V**

**A-25471**

**F7**

**F9**

**F5**

**F3**

**F9A**

**F1**

**F4**

**F6**

**F2**

**A.S.**

**WARNING — FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A  
FUSE OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

SOUND SPEECH (WHEN USED)

LIGHTBOX ILLUMINATION

**8 AMP.**

**250V. SLO–BLO**

PLAYFIELD ILLUMINATION

**8 AMP.**

**250V. SLO–BLO**

CONTROLLED LAMPS

**10 AMP.**

**250V. NORMAL–BLO**

SOLENOIDS (+24V DC)

**8 AMP.**

**250V. SLO–BLO**

DISPLAY (32V AC)

**0.25 AMP.**

**250V. SLO–BLO**

POWER SUPPLY (A2)

**5 AMP.**

**250 V. SLO–BLO**

SOUND POWER SUPPLY (A6)

**0.50 AMP.**

**250V. NORMAL–BLO**

PRIMARY POWER

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**WARNING —** FOR CONTINUED PROTEC-  
TION AGAINST FIRE HAZARD REPLACE ONLY WITH A FUSE OF THE SAME TYPE AND HAVING THE SAME ELECTRICAL RATING.

NOT USED

10 AMP

250V. SLO-BLO

8 AMP

250V. SLO-BLO

10 AMP

250V. SLO-BLO

8 AMP

250V. SLO-BLO

0.25 AMP

250V. SLO-BLO

5 AMP

250 V. SLO-BLO

0.50 AMP

250V. NORMAL-BLO

5 AMP SLO-BLO/115 VAC

2.5 AMP SLO-BLO/230 VAC

**SOUND POWER SUPPLY (A5)**

**0.50 AMP NORMAL-BLO**

**32 V**

**POWER SUPPLY (A2)**

**6.25 AMP SLO-BLO**

**250 V**

**DISPLAYS (32V AC)**

**0.25 AMP SLO-BLO**

**250 V**

**SOLENOIDS (+24V DC)**

**8 AMP SLO-BLO**

**250 V**

**CONTROLLED LAMPS**

**10 AMP SLO-BLO**

**32 V**

**PLAYFIELD ILLUMINATION**

**5 AMP SLO-BLO**

**250 V**

**DISPLAY FILAMENT**

**1 AMP NORMAL BLO**

**32 V**

**WARNING - FOR CONTINUED PROTECTION  
AGAINST FIRE HAZARD REPLACE ONLY WITH A  
FUSE OF THE SAME TYPE AND HAVING THE SAME  
ELECTRICAL RATING.**

**F1**

**F2**

**F3**

**F4**

**F5**

**F6**

**F9**

**F9A**

**PRIMARY POWER**

**5 AMP SLO-BLO/115 VAC**

**2.5 AMP SLO-BLO/230 VAC**

**LIGHTBOX ILLUMINATION**

**0.50 AMP SLO-BLO**

**250 V**

**F8**

**F7**

**F15**

**F7**

**F6**

**F5**

**F4**

**F3**

**F2**

**F1**

**F15**

**F7**

**F6**

**F5**

**25950**

**F4**

**F3**

**24174-1**

**F2**

**F1**

A-24483

**F8**

**F8**

Fonts used: News Gothic Std.

**Cards status:**

A-25470 Fuse card confirmed (Victory).

A-24421 Fuse card confirmed (Ice Fever).

A-25029 Fuse card confirmed (Hollywood Heat).

A-25096 Fuse card confirmed (Goldwings).

A-25471 French fuse card confirmed (Victory).

Fuse card labelled as “A.S.” needed to verify (Alien Star).

A-25950 Fuse card confirmed (Hot Shots).

A-24174-1 Fuse card confirmed (Touchdown).

A-24483 Fuse card confirmed (Chicago Cubs).

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.