ALI SELF TEST DISPLAY NUMBERS

**SOLENOID IDENTIFICATION**

**SOLENOID NO. SOLENOID LOCATION**

01 . . . . . . . . . RIGHT SLING-SHOT

02 . . . . . . . . . LEFT SLING-SHOT

03 . . . . . . . . . KNOCKER

04 . . . . . . . . . TOP (3) SAUCERS

05 . . . . . . . . . LEFT THUMPER

06 . . . . . . . . . MIDDLE THUMPER

07 . . . . . . . . . RIGHT THUMPER

08 . . . . . . . . . LEFT BANK TARGET

09 . . . . . . . . . OUT-HOLE

10 . . . . . . . . . OPEN

11 . . . . . . . . . GENERAL ILLUMINATION RELAY

12 . . . . . . . . . OPEN

13 . . . . . . . . . LOWER BANK TARGET

14 . . . . . . . . . MIDDLE RIGHT SAUCER

15 . . . . . . . . . FLIPPERS (RIGHT & LEFT)

16 . . . . . . . . . OPEN

17 . . . . . . . . . OPEN

18 . . . . . . . . . OPEN

19 . . . . . . . . . COIN LOCK-OUT

20 thru 29 . . . SOUND

**SWITCH IDENTIFICATION**

**SWITCH SWITCH  
 NO. SWITCH LOCATION NO. SWITCH LOCATION**

01 CHUTE SEE 21 TOP BANK, RIGHT TARGET

02 CHUTE DIAGRAM 22 LEFT BANK, BOTTOM TARGET

03 CHUTE BELOW 23 LEFT BANK, MIDDLE TARGET

04 NOT-USED 24 LEFT BANK, TOP TARGET

05 BOTTOM R.O. BUTTON 25 STAND-UP TARGET “G”

06 CREDIT BUTTON 26 STAND-UP TARGET “R”

07 TILTS 27 STAND-UP TARGET “E”

08 SLAM & VIB. TILTS 28 STAND-UP TARGET “A”

09 TOP-LEFT R.O. BUTTON 29 STAND-UP TARGET “T”

10 NOT-USED 30 TOP LEFT SAUCER

11 TWO MIDDLE R.O. BUTTONS 31 TOP MIDDLE SAUCER

12 RIGHT THUMPER 32 TOP RIGHT SAUCER

13 LEFT THUMPER 33 OUT-HOLE

14 MIDDLE THUMPER 34 RIGHT OUT-LANE

15 RIGHT SLING-SHOT 35 LEFT OUT-LANE

16 LEFT SLING-SHOT 36 RIGHT RETURN LANE

17 NOT-USED 37 LEFT RETURN LANE

18 NOT-USED 38 MIDDLE RIGHT SAUCER

19 TOP BANK, LEFT TARGET 39 MIDDLE LEFT R.O. WIRE

20 TOP BANK, MIDDLE TARGET 40 NOT-USED

**SW1 SW2 SW3 SW2 SW3**

3-CHUTE 2-CHUTE

DOOR DOOR

NOTE: FLIPPER BUTTON CABINET SWITCHES DO NOT APPEAR ON TEST

12C-264-7

**SELF TEST**

**BUTTON LOCATED INSIDE OF COIN DOOR**

**NO. OF**

**TIMES PUSHED TEST DESCRITION**

1 BURN IN All outputs tested.

2 LAMPS All feature lamps will  
 flash on & off.

3 DISPLAY All digits display  
 000000 thru 999999  
 then No. 8 shifts from  
 left to right.

4 SOLENOIDS Continuous sequence  
 of solenoids pulsed,  
 then all sounds pulsed.  
 (Solenoid driver tran-  
 sistor “Q” number dis-  
 played as solenoid is  
 pulsed.)

5 SWITCHES Switch I.D. No. dis-  
 (Flashing 0 if all plays if closed (See  
 switches open) chart for switch I.D.  
 No.)

6 To 23 THRESHOLD & See Operating Manual  
 BOOKKEEPING

}

HINGE

SIDE

HINGE

SIDE

Font used: HelveticaNeueLT Std Thin, Helvetica, Helvetica-Condensed, Futura Std ExtraBold

Self Test card 12C-264-7 (size 140 x 280 mm) confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.