METEOR SELF TEST DISPLAY NUMBERS

**SWITCH IDENTIFICATION**

**SWITCH SWITCH  
 NO. SWITCH LOCATION NO. SWITCH LOCATION**

01 .... COIN CHUTE SEE 18 .... OPEN

02 .... COIN CHUTE DRWG. 19-21 ... 3-BANK DROP TARGET

03 .... COIN CHUTE BELOW (TOP LEFT)

04 .... STAND-UP TARGET 22-24 ... 3-BANK DROP TARGET

05 .... SPIN TARGET (LEFT CENTER)

06 .... CREDIT BUTTON 25 .... OPEN

07 .... TILTS 26 .... OPEN

08 .... SLAM & VIB. TILTS 27-32 ... 6-BANK DROP TARGETS

09-11 ... 3-BANK DROP TARGET 33 .... OUT-HOLE

(RIGHT) 34 .... RIGHT OUT-LANE

12 .... BUMPER (UPPER RIGHT) 35 .... LEFT OUT-LANE

13 .... BUMPER (UPPER LEFT) 36 .... RIGHT RETURN LANE

14 .... THUMPER BUMPER 37 .... LEFT RETURN LANE

15 .... RIGHT SLING-SHOT 38 .... ROLL-OVER BUTTON (UPPER)

16 .... LEFT SLING-SHOT 39 .... ROLL-OVER BUTTON (CENTER)

17 .... OPEN 40 .... ROLL-OVER BUTTON (LOWER)

**SW1 SW2 SW3 SW2 SW3**

3-CHUTE 2-CHUTE

DOOR DOOR

NOTE: FLIPPER BUTTON CABINET SWITCHES DO NOT  
 APPEAR ON TEST

12C-264-4

**SOLENOID IDENTIFICATION**

**SOLENOID NO. SOLENOID LOCATION**

01 . . . . . . . . . . THUMPER BUMPER

02 . . . . . . . . . . LEFT SLING-SHOT

03 . . . . . . . . . . KNOCKER

04 . . . . . . . . . . 3-BANK DROP TARGET  
 (LEFT BOTTOM)

05 . . . . . . . . . . 3-BANK DROP TARGET  
 (LEFT TOP)

06 thru 11 . . . . 6-BANK DROP TARGETS

12 . . . . . . . . . . 6-BANK DROP TARGET  
 (Reset)

13 . . . . . . . . . . 3-BANK DROP TARGET  
 (Right)

14 . . . . . . . . . . RIGHT SLING-SHOT

15 . . . . . . . . . . FLIPPERS

16 . . . . . . . . . . OUT-HOLE

19 . . . . . . . . . . COIN LOCK-OUT

20 thru 29 . . . . SOUND

**SELF TEST**

**BUTTON LOCATED INSIDE OF COIN DOOR**

**NO. OF**

**TIMES PUSHED TEST DESCRITION**

1 BURN IN All outputs tested.

2 LAMPS All feature lamps will  
 flash on & off.

3 DISPLAY All digits display   
 000000 thru 999999  
 then No. 8 shifts from  
 left to right.

4 SOLENOIDS Continuous sequence  
 of solenoids pulsed,  
 then all sounds pulsed.  
 (Solenoid driver tran-  
 sistor “Q” number dis-  
 played as solenoid is  
 pulsed.)

5 SWITCHES Switch I.D. No. dis-   
 (Flashing 0 if all plays if closed (See  
 switches open) chart for switch I.D.  
 No.)

6 To 23 THRESHOLD & See Operating Manual  
 BOOKKEEPING

{

HINGE

SIDE

HINGE

SIDE

Font used: HelveticaNeueLT Std Thin, Helvetica, Helvetica-Condensed, Futura Std ExtraBold

Self Test card 12C-264-4 (size 140 x 280 mm) confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.