SEAWITCH SELF TEST DISPLAY NUMBERS

**SOLENOID IDENTIFICATION**

**SOLENOID NO. SOLENOID LOCATION**

1 . . . . . . . . . LEFT THUMPER

2 . . . . . . . . . TOP THUMPER

3 . . . . . . . . . KNOCKER

4 . . . . . . . . . CENTER BANK TARGET

5 . . . . . . . . . OPEN

6 . . . . . . . . . LEFT SLING-SHOT

7 . . . . . . . . . RIGHT SLING-SHOT

8 . . . . . . . . . LEFT BANK TARGET

9 . . . . . . . . . RIGHT THUMPER

10 . . . . . . . . . OPEN

11 . . . . . . . . . OPEN

12 . . . . . . . . . OPEN

13 . . . . . . . . . TOP RIGHT BANK TARGET

14 . . . . . . . . . OUT-HOLE

15 . . . . . . . . . FLIPPERS (4)

16 . . . . . . . . . OPEN

17 . . . . . . . . . OPEN

18 . . . . . . . . . OPEN

19 . . . . . . . . . COIN LOCK-OUT

20 thru 29 . . . SOUND

**SWITCH IDENTIFICATION**

**SWITCH SWITCH  
 NO. SWITCH LOCATION NO. SWITCH LOCATION**

01 Coin Chute 21 Center Bank Target (No. 1)

02 Coin Chute See drawing 22 Center Bank Target (No. 2)

03 Coin Chute Below 23 Center Bank Target (No. 3)

04 Top Roll-Over Button 24 Center Bank Target (No. 4)

05 Spinning Target 25 Runway Roll-Over Button

06 Credit Button 26 Not Used

07 Tilts 27 Not Used

08 Slam & Vib. Tilts 28 Not Used

09 Top Thumper 29 Top Right Bank Target (No.1)

10 Left Thumper 30 Top Right Bank Target (No.2)

11 Not Used 31 Top Right Bank Target (No.3)

12 Left Sling-Shot 32 Top Right Bank Target (No.4)

13 Right Sling-Shot 33 Out-Hole

14 Right Thumper 34 Left Out-Lane

15 Not Used 35 Right Out-Lane

16 Not Used 36 Left Return Lane

17 Stand-Up Target (Top Right) 37 Right Return Lane

18 Stand-Up Target (Top Left) 38 Left Bank Target (No.1)

19 Stand-Up Target (Top Left Mid.) 39 Left Bank Target (No.2)

20 Stand-Up Target (Top Left Low.) 40 Left Bank Target (No.3)

**SW1 SW2 SW3**

**GERMANY**

NOTE: FLIPPER BUTTON CABINET SWITCHES DO NOT APPEAR ON TEST

12A-264-8

**SELF TEST**

BUTTON LOCATED INSIDE OF COIN DOOR

**NO. OF**

**TIMES PUSHED TEST DESCRITION**

1 BURN IN All outputs tested.

2 LAMPS All feature lamps will  
 flash on & off.

3 DISPLAY All digits display 000000  
 thru 999999 then No. 8  
 shifts from left to right.

4 SOLENOIDS Continuous sequence of  
 solenoids pulsed, then  
 all sounds pulsed.  
 (Solenoid driver transis-  
 tor “Q” number dis-  
 played as solenoid is  
 pulsed.)

5 SWITCHES Switch I.D. No. displays  
 (Flashing 0 if all if closed (See chart for  
 switches open) switch I.D. No.)

6 To 23 THRESHOLD & See Operating Manual  
 BOOKKEEPING

}

HINGE

SIDE

Font used: HelveticaNeueLT Std Thin, Helvetica, Helvetica-Condensed, Futura Std ExtraBold

Self Test card 12A-264-8 (size 140 x 280 mm) confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.