GENERAL INSTRUCTIONS FOR TARGET GALLERY

1. INSTALLATION:  
   • Fasten the 4 legs to cabinet with furnished bolts.  
   • Install the back-box on the cabinet with furnished bolts and attach all discon-  
    nect jacks.  
   • Put the furnished 13/16" diameter steel balls into opening of ball return trough  
    which is accessible above the cash box.  
   • Level the game and adjust the front tilt switch.  
   • Plug the line cord into A.C. only, 60 cycles, 115 volts; the power is controlled  
    by a toggle switch located under the front part of the game.
2. VOLTAGE CONTROL: In low voltage areas (105 volts or less) an additional  
   boost in the output voltage of the transformer can be obtained by inserting the  
   transformer voltage control fuse into the "LOW LINE" fuse position.
3. SCORE REPLAY CONTROL JACK is located on the 100 score drum unit. It is  
   also used as a control for the "PLAY AGAIN" feature on the non-replay model.
4. TO SERVICE TARGET PANEL:   
   • Disconnect the small jack on the back door.  
   • Remove top two screws holding canopy to cabinet.  
   • Trip all animals and slide target panel out.

10136 W. PACIFIC AVENUE FRANKLIN PARK, ILLINOIS

Midway Mfg. Co.

• Rabbits and Squirrels  
 score as indicated. Hit-  
 ting both targets with  
 one ball will score both.

• Bat ball EARLY to hit  
 targets at left side.

• Bat ball LATE to hit  
 targets at right side.

10c – 20 BALLS per game

• Rabbits and Squirrels  
 score as indicated. Hit-  
 ting both targets with  
 one ball will score both.

• Bat ball EARLY to hit  
 targets at left side.

• Bat ball LATE to hit  
 targets at right side.

5c – 20 BALLS per game

1900 – 1 replay 3200 – 4 replays

2000 – 2 replays 3600 – 5 replays

2600 – 3 replays 4200 – 6 replays

REPLAYS

*LOWER pockets score 1 replay  
when SPECIAL is lit.*

*— Press Coin Reject Button —*

TG-30

2000 – 1 replay 3300 – 4 replays

2300 – 2 replays 3600 – 5 replays

2600 – 3 replays 4300 – 6 replays

REPLAYS

*LOWER pockets score 1 replay  
when SPECIAL is lit.*

*— Press Coin Reject Button —*

TG-24

– 1 replay – 4 replays

– 2 replays – 5 replays

– 3 replays – 6 replays

REPLAYS

*LOWER pockets score 1 replay  
when SPECIAL is lit.*

*— Press Coin Reject Button —*

TG-40

2100 – 1 replay 3300 – 4 replays

2300 – 2 replays 3600 – 5 replays

2600 – 3 replays 4300 – 6 replays

REPLAYS

*LOWER pockets score 1 replay  
when SPECIAL is lit.*

*— Press Coin Reject Button —*

TG-34

PLAY AGAIN IFSCORE OF 1800  
IS MADE

*— Press Coin Reject Button —*

PLAY AGAIN IFSCORE OF 1700  
IS MADE

*— Press Coin Reject Button —*

PLAY AGAIN IFSCORE OF 2000  
IS MADE

*— Press Coin Reject Button —*

PLAY AGAIN IFSCORE OF 1900  
IS MADE

*— Press Coin Reject Button —*

PLAY AGAIN IFSCORE OF \_\_\_\_\_  
IS MADE

*— Press Coin Reject Button —*

PLAY AGAIN IFSCORE OF 2100  
IS MADE

*— Press Coin Reject Button —*

Fonts used: Futura BdCn BT, Futura Hv BT, Futura-Thin, Futura Std Medium, BrushScriptOpti

Card size: 213x200mm, 57x82mm, 29x82mm

**Card status:**

General Instructions card confirmed.

5c instructions card confirmed.

10c instructions card confirmed.

TG-24 score card confirmed.

TG-30 score card confirmed.

TG-34 score card confirmed.

TG-40 score card confirmed.

Play Again at 1700 card confirmed.

Play Again at 1800 card confirmed.

Play Again at 1900 card confirmed.

Play Again at 2000 card confirmed.

Play Again at 2100 card confirmed.

Play Again at blank card confirmed.

If you have any more information, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.