**INSTRUCTION FOR USE OF BILL ACCEPTOR/UPSTACKER OPTION**

**MOUNTING A BILL ACCEPTOR**

1. REMOVE AND RETAIN HEX NUTS A, B;  
 SCREWS C, D, E, F, H, I, J, AND PLASTIS  
 SPACERS ON C, F.

2. REMOVE TOP COVER PLATE.

3. PUT THE PLASTIC SPACERS FROM C, F  
 ONTO H, I. (KEEP THEM FOR IN CASE USING  
 AN UPSTACKER)

4. MOUNT BILL ACCEPTOR OVER STUDS A, B.

5. SECURE USING HEX NUTS A, B AND  
 SCREWS H, I.

**MOUNTING AN UPSTACKER**

1. REMOVE AND RETAIN SCREWS C, F, G, H, I, J;  
 HEX NUTS K, L; AND SPACERS ON K, L.

2. REMOVE BOTTOM COVER PLATE.

3. PUT THE PLASTIC SPACER ONTO K, L AS  
 IT WAS.

4. MOUNT UPSTACKER OVER STUDS K, L.

5. PLACE GROUND WIRE COMING FROM THE  
 UPSTACKER UNIT ON STUD L.

6. SECURE USING SCREWS C, F AND HEX NUTS  
 K, L.

A B

TOP COVER PLATE

D E

C F

G J

H I

BOTTOM COVER PLATE

K L

**INSTRUCTION FOR USE OF BILL ACCEPTOR/UPSTACKER OPTION**

**MOUNTING A BILL ACCEPTOR**

1. REMOVE AND RETAIN HEX NUTS A, B;  
 SCREWS C, D, E, F, H, I, J, AND PLASTIS  
 SPACERS ON C, F.

2. REMOVE TOP COVER PLATE.

3. PUT THE PLASTIC SPACERS FROM C, F  
 ONTO H, I. (KEEP THEM FOR IN CASE USING  
 AN UPSTACKER)

4. MOUNT BILL ACCEPTOR OVER STUDS A, B.

5. SECURE USING HEX NUTS A, B AND  
 SCREWS H, I.

**MOUNTING AN UPSTACKER**

1. REMOVE AND RETAIN SCREWS C, F, G, H, I, J;  
 HEX NUTS K, L; AND SPACERS ON K, L.

2. REMOVE BOTTOM COVER PLATE.

3. PUT THE PLASTIC SPACER ONTO K, L AS  
 IT WAS.

4. MOUNT UPSTACKER OVER STUDS K, L.

5. PLACE GROUND WIRE COMING FROM THE  
 UPSTACKER UNIT ON STUD L.

6. SECURE USING SCREWS C, F AND HEX NUTS  
 K, L.

A B

TOP COVER PLATE

D E

C F

G J

H I

BOTTOM COVER PLATE

K L

Used fonts: HelveticaNeueLT Std Med, HelveticaNeueLT Std Med Cn

Card size: 82.5x92mm.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.