###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8A

###### IMPORTANT NOTE

WHEN USING DRIVER  
BOARDS WITH PADS FOR  
SWITCH MATRIX SERIES  
RESISTORS R204 THRU  
R211 (EARLIER BOARDS),  
THOSE COMPONENTS  
MUST BE ZERO-OHM OR  
BE REPLACED WITH  
JUMPER WIRES.

###### 500-8

###### IMPORTANT NOTE

WHEN USING DRIVER BOARDS WITH PADS FOR SWITCH MATRIX SERIES RESISTORS R196 THRU R211 (EARLIER BOARDS), THOSE COMPONENTS MUST BE ZERO-OHM OR  
BE REPLACED WITH JUMPER WIRES.

Fonts used: Tremolo

Card size: 50x59mm

**Cards status:**

Card 500-8 is confirmed, but is later replaced by 500-8A because it had wrong information  
about the resistor jumpers. Card 500-8 is replaced by 500-8A.

Card 500-8A is confirmed. (correct jumper information).

A similar card is STD-A714.

If you have any other information about these cards,

please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.