TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

TO REMOVE BACKGLASS:

WITH BACK DOOR REMOVED,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 41A

Fonts used: Franklin Gothic Medium, HelveticaNeueLT Std Ext.

Card size: 3.5 x 2 inch, 89x50mm

**Cards status:**

Serviceman label STD-41A confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.