TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

TO REMOVE BACKGLASS:

WITH BACK DOOR OPEN,  
PULL BACK ON BRACKETS  
AT INSIDE TOP OF LITE BOX.

FROM THE FRONT OF GAME,  
LIFT GLASS UP AND OUT.

###### SERVICEMAN

###### STD. 47A

Fonts used: Franklin Gothic Medium, HelveticaNeueLT Std Ext.

Card size: 89x50mm

**Cards status:**

Serviceman label STD-47A confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.