SWITCH ADJUSTMENT

BEFORE ADJUSTING SWITCHES, MAKE CERTAIN  
THE SCREWS HOLDING THE SWITCH STACKS  
ARE DOWN TIGHTLY. BAKELITE SPACERS IN  
THE SWITCH STACKS, DUE TO EXCESSIVE  
MOISTURE, HAVE OCCASIONALLY SHRUNK BY  
DRYING OUT, CAUSING POOR ADJUSTMENT.

STD. 50A

SWITCH ADJUSTMENT

BEFORE ADJUSTING SWITCHES, MAKE CERTAIN  
THE SCREWS HOLDING THE SWITCH STACKS  
ARE DOWN TIGHTLY. BAKELITE SPACERS IN  
THE SWITCH STACKS, DUE TO EXCESSIVE  
MOISTURE, HAVE OCCASIONALLY SHRUNK BY  
DRYING OUT, CAUSING POOR ADJUSTMENT.

STD. 50A

SWITCH ADJUSTMENT

BEFORE ADJUSTING SWITCHES, MAKE CERTAIN  
THE SCREWS HOLDING THE SWITCH STACKS  
ARE DOWN TIGHTLY. BAKELITE SPACERS IN  
THE SWITCH STACKS, DUE TO EXCESSIVE  
MOISTURE, HAVE OCCASIONALLY SHRUNK BY  
DRYING OUT, CAUSING POOR ADJUSTMENT.

STD. 50A

Fonts used: HelveticaNeue, Century Schoolbook

Card size: 5 x 2.5 inch, 126x63mm

**Cards status:**

Switch Adjustment label STD-50A confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.