**WARNING**

FOR SAFETY AND PROPER  
GAME OPERATION, GAME  
MUST BE PLUGGED IN TO  
A PROPERLY GROUNDED OUTLET  
117 VAC, 60 HZ.

**STD-615**

**WARNING**

FOR SAFETY AND PROPER  
GAME OPERATION, GAME  
MUST BE PLUGGED IN TO  
A PROPERLY GROUNDED OUTLET  
117 VAC, 60 HZ.

**STD-615**

Card status:

Used fonts: Futura Hv BT, Helvetica LT Std Cond, Futura Md BT

Card size: 146x82mm.

STD-615 Outlet Warning label confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.