**MASTER COMMAND**

**Zero Restore Auto Cycle  
 Audit Factory Test Mode  
 Totals Settings**

**NOT USED**

**MASTER COMMAND PROCEDURE**

1. IN GAME OVER, SET COIN DOOR  
   TOGGLE SWITCH TO MANUAL  
   DOWN AND DEPRESS ADVANCE.  
   (DISPLAYS GO BLANK)  
   LEAVE COIN DOOR OPEN.
2. SET MASTER COMMAND  
   SWITCH FOR DESIRED  
   COMMAND AS INDICATED.
3. DEPRESS MASTER  
   COMMAND ENTER.  
   (LEDS BLINK ONCE)
4. FOR AUTO CYCLE, SET  
   SWITCH TO AUTO UP  
   AND DEPRESS ADVANCE.
5. TO RETURN TO GAME OVER,  
   TURN GAME OFF AND BACK ON.

MASTER

COMMAND

ENTER

DIAGNOSTIC  
(USE FOR TROUBLE  
SHOOTING ONLY)

8

7

6

5

4

3

2

1

ON

8

7

6

5

4

3

2

1

ON

8

7

6

5

4

3

2

1

ON

STD-617

Card status:

Used fonts: Helvetica CE, Century

Card size: 67x145mm.

STD-617 Master Command card confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.