**Special Adjustment Index  
Pos. Motor Sw.**

Motor run sw. wire colors  
Orange/Green and Yellow  
should make before 100,000  
reset cont. sw. wire colors  
Red/Blue and Green/White  
break.

**Std. 66**

**Special Adjustment Index  
Pos. Motor Sw.**

Motor run sw. wire colors  
Orange/Green and Yellow  
should make before 100,000  
reset cont. sw. wire colors  
Red/Blue and Green/White  
break.

**Std. 66**

Fonts used: Rockwell, Century

Size: 44x30mm

Std. 66 Motor Switch label confirmed.

If you have more labels like this, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.