STD-936-2

AUXILIARY  
DRIVER/POWER  
ASSEMBLY

NOT USED  
W6

25V.D.C A/C SELECT

F2

2.5 A.S.B. F2A 25 V.D.C. COIL-BRN

5 A.S.B. F2C FLASH LAMP-ORG

2.5 A.S.B. F4 50 V.D.C. COIL-YEL/VIO

2 A.S.B. F5

50 V.D.C.  
RIGHT FLIPPERS-BLU/YEL

50 V.D.C.  
LEFT FLIPPERS-GRY/YEL

2 A.S.B. F6

F8

7 A.S.B.

25 V.A.C.

4 A.S.B. F7 50 V.A.C.

F3

RED/WHT — 5 A.S.B.

25 V.D.C. COIL

F1

RED — 2.5 A.S.B.

25 V.D.C.

STD-936-1

AUXILIARY  
DRIVER/POWER  
ASSEMBLY

NOT USED  
W6

25V.D.C A/C SELECT

F2

2.5 A.S.B. F2A 25 V.D.C. COIL-BRN

5 A.S.B. F2C FLASH LAMP-ORG

2.5 A.S.B. F4 50 V.D.C. COIL-YEL/VIO

2 A.S.B. F5

50 V.D.C.  
RIGHT FLIPPERS-BLU/YEL

50 V.D.C.  
LEFT FLIPPERS-GRY/YEL

2 A.S.B. F6

F8

7 A.S.B.

25 V.A.C.

4 A.S.B. F7 50 V.A.C.

F3

RED/WHT — 2.5 A.S.B.

25 V.D.C. COIL

F1

RED — 2.5 A.S.B.

25 V.D.C.

STD-936

AUXILIARY  
DRIVER/POWER  
ASSEMBLY

NOT USED  
W6

25V.D.C A/C SELECT

F2

2.5 A.S.B. F2A 25 V.D.C. COIL-BRN

5 A.S.B. F2C FLASH LAMP-ORG

2 A.S.B. F4 50 V.D.C. COIL-YEL/VIO

2 A.S.B. F5

50 V.D.C.  
RIGHT FLIPPERS-BLU/YEL

50 V.D.C.  
LEFT FLIPPERS-GRY/YEL

2 A.S.B. F6

F8

7 A.S.B.

25 V.A.C.

4 A.S.B. F7 50 V.A.C.

F3

RED/WHT — 2.5 A.S.B.

25 V.D.C. COIL

F1

RED — 2.5 A.S.B.

25 V.D.C.

Elvira, standard Taxi, F4 adjusted to 2.5A Earthshaker, F3 adjusted to 5A

Fonts used: Futura Md BT.

STD-936 standard fuse card confirmed (size 82x114mm).

STD-936-1 has F4 adjusted to 2.5A as is confirmed in Taxi.

STD-936-2 has F3 adjusted to 5A as is confirmed in Earthshaker.

If you have any more fuse labels, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.