###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

###### STD-A714

###### IMPORTANT:

WHEN REPLACING DRIVER  
BOARD, MAKE SURE THAT  
W9 - W16 (R204 - R211)  
ARE ZERO-OHM RESISTORS  
OR WIRE JUMPERS.

Fonts used: Tremolo

Card size: 50x56mm

**Cards status:**

Card STD-A714 is confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.