**PLEASE NOTE**

THE MPU AND RECTIFIER BOARDS IN  
OTHER BALLY PINBALL GAMES ARE  
INTERCHANGEABLE PROVIDED THE  
FOLLOWING CHANGES ARE MADE.

TO MODIFY AN EXISTING MPU FOR USE  
IN A BABY PAC-MAN GAME R113 MUST  
BE CHANGED TO A 1N4148 DIODE.

TO UPDATE THE RECTIFIER BOARD CR5,  
CR6, CR7, AND CR8 MUST BE REPLACED  
WITH 6AMP DIODES. (MOTOROLA  
MR-751, GENERAL INSTRUMENT P600B  
OR BALLY E-587-32)

*REFER TO GAME MANUAL SCHEMATICS*

Font used: HelveticaNeueLT Std Med

Size: 210x190mm

**Cards status:**

Please Note label confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.