**TO REMOVE BACKBOX**

**1) DISCONNECT CABINET &  
 PLAYFIELD CABLES,  
 AND GROUND STRAP.**

**2) REMOVE TOP WOOD SCREW  
 AND PIVOT WOOD BLOCK.**

**3) SLIDE ENTIRE BACKBOX  
 TO RIGHT, OFF HINGE.**

Fonts used: News Gothic MT Std.

**Cards status:**

To Remove Backbox card confirmed (no card number).

The card on the right is a scan of the original (older type) card.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.