25 SHOTS PER GAME

SCORE OF

2900

1 REPLAY

25 SHOTS PER GAME

SCORE OF

2800

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3100

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3000

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3300

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3200

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3500

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3400

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3700

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3600

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3900

1 REPLAY

25 SHOTS PER GAME

SCORE OF

3800

1 REPLAY

25 SHOTS PER GAME

25 SHOTS PER GAME

SCORE OF

4000

1 REPLAY

25 SHOTS PER GAME

SCORE OF

2900

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

2800

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3100

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3000

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3300

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3200

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3500

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3400

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3700

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3600

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3900

1 EXTENDED PLAY

25 SHOTS PER GAME

SCORE OF

3800

1 EXTENDED PLAY


25 SHOTS PER GAME

SCORE OF

4000

1 EXTENDED PLAY

25 SHOTS PER GAME



RODEO SHOOTING GALLERY

**ADJUSTMENTS**

HI – SCORE

ADJ.

LOCATED – LEFT SIDE

OF BACKRACK

SOCKET

000 - - 500

900 - - 400

800 - - 300

700 - - 200

600 - - 100

PLUGS

YEL

RED

BRN

GAME ADJ.

PLACE THE PLUG IN THE  
"REPLAY" POSITION TO  
GIVE THE PLAYER ONE  
REPLAY FOR HI-SCORE.

PLACE THE PLUG IN THE  
"EXTENDED PLAY" POSITION  
TO GIVE THE PLAYER AN  
EXTENDED PLAY FOR HI-SCORE.

GAME ADJ.

REPLAY

EXTENDED

PLAY

(1100 TO 2000)

(2100 TO 2000)

(3100 TO 4000)

ORANGE

PLACE THE PLUG  
IN THE SCORE  
THAT YOU WISH  
TO AWARD A REPLAY  
OR EXTENDED PLAY  
WHEN THE PLAYER  
REACHES THAT  
SCORE.

EXAMPLES:

YELLOW WIRE INTO 400 POS. SCORES AT 1400.

RED WIRE INTO 800 POS. SCORES AT 2800.

BROWN WIRE INTO 200 POS. SCORES AT 3200.

USE ONE PLUG ONLY.

LOCATED – TOP LEFT  
CORNER OF BACKRACK

EXTENDED PLAY

SHOT ADJ.

GAME OVER

SHOT ADJ.

LOCATED ON

LEFT SIDE

OF BACKRACK

15

20

25

15

20

25

MISS SHOT ADJUSTMENTS

MISS SHOT ADJUSTMENTS

THERE ARE NONE IN "REG."  
POSITION.

THERE IS A POSSIBILITY  
OF ONE OR MORE IN "LESS"  
POSITION.

THERE IS A POSSIBILITY  
OF SEVERAL IN THE "MORE"  
POSITION.

BLUE–YEL.

REG.

NO MISS

BLK–GRN

LESS

1 MISS

MORE


2 MISS

LOCATED ON BACK - DOOR

TOP RIGHT CORNER.

25 SHOTS PER GAME  
WHEN PLUG IS IN THIS  
POSITION.

15 SHOTS PER EXTENDED  
PLAY WHEN PLUG IS IN  
THIS POSITION.



RODEO SHOOTING GALLERY

1st. CAM

A–1 – MOTOR RUN.

A–2 – COMMON TO TRIGGER SWITCH.

A–3 – TO CREDIT RESET RELAY.

A–4 – TO SLIDE BANK RESET RELAY.

A–5 – TO GAME OVER RELAY.

A–6 – TO FLASH–O–MATIC CLUTCH COIL.

2nd. CAM

A–7 – TO 25¢ RELAY FOR CREDIT STEP-UP.

A–8 – TO FLASH–O–MATIC DISC FOR SCORE.

1st. CAM

B–1 – CREDIT UNIT RESET & SHOT UNIT RESET.

B–2 – SHOT COUNT STEP–UP & EXTENDED PLAY LITE RELAY.

1st. CAM

C–1 – ANTI–CHEAT RELAY.

C–2 – TO 10¢ RELAY FOR CREDIT STEP–UP.

C–3 – TO TARGET RESET COILS.

C–4 – SLIDE BANK RESET COIL.

1st. CAM

D–1 – 30V. BREAK FOR TRIGGER RELAY.

D–2 – TO FLASH–O–MATIC DISC FOR SCORE.

1st. CAM

E–1 – 30 VOLT BREAK FOR RELAYS.

E–2 – FLASH–O–MATIC CLUTCH COIL TO CHANGE SCORE VALUE.

E–3 – 30V. BREAK FOR HIT RELAY COILS.

2nd. CAM

E–4 – MYSTERY TARGET SCORE.

3rd. CAM

E–5 – TO 25¢ RELAY FOR CREDIT STEP–UP.

E–6 – TO FLASH–O–MATIC DISC FOR SCORE.

4th. CAM

E–7 – TO START RELAY FOR SCORE RESET.

E–8 – TO FLASH–O–MATIC DISC FOR SCORE.

Fonts used: Futura Hv BT, AlternateGothicEF, News Gothic Std, AlternateGotNo3D, News Gothic Demi

Score card size: 76x51mm

Adjustments and motor cams pages are full sheets (A4 or letter).

**Cards status:**

All score cards confirmed.

Adjustments sheet confirmed.

Motor cams sheet confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.