**INSTRUCTIONS**

**3 BALLS PER PLAY**

POINTS ARE SCORED AS INDICATED.

HITTING LIT BASEBALL TARGETS OR LIT TOP ROLLOVERS PLACES MAN  
 ON CORRESPONDING BASE.

ROLLOVER BUTTONS SCORE 10 POINTS WHEN LIT.

MATCHING LAST NUMBER IN SCORE TO NUMBER THAT APPEARS  
 ON BACK GLASS AFTER GAME IS OVER AWARDS ONE REPLAY.

BALL IN PLAY

290

B-12805

**INSTRUCTIONS**

**5 BALLS PER PLAY**

POINTS ARE SCORED AS INDICATED.

HITTING LIT BASEBALL TARGETS OR LIT TOP ROLLOVERS PLACES MAN  
 ON CORRESPONDING BASE.

ROLLOVER BUTTONS SCORE 10 POINTS WHEN LIT.

MATCHING LAST NUMBER IN SCORE TO NUMBER THAT APPEARS  
 ON BACK GLASS AFTER GAME IS OVER AWARDS ONE REPLAY.

BALL IN PLAY

290

B-12805

**SCORE CARDS ARE LISTED FROM LIBERAL TO CONSERVATIVE**

**CARDS MARKED \* ARE RECOMMENDED.**

**ADJUSTMENT PLUG LOCATION**

**INSIDE LIGHTBOX** ! **PT. SCORE ADJ. & RUNS SCORE ADJ.**

**BOTTOM PANEL** ! **1ST & 2ND CHUTE ADJ., 3RD CHUTE ADJ. & 3-5  
BALL ADJ.**

**5 BALL PLAY**

**A-12812 – 4700, 6100, 6900**

**A-12813 – 4800, 6200, 7000**

**A-12814 – 4900, 6300, 7100**

**\* A-12526 – 5000, 6400, 7200**

**A-12815 – 5100, 6500, 7300**

**A-12527 – 5200, 6600, 7400**

**A-12816 – 5300, 6700, 7500**

**A-12822 – 16, 22, 28**

**A-12823 – 17, 22, 28**

**\* A-12824 – 18, 23, 29**

**A-12825 – 19, 23, 28**

**A-12826 – 19, 24, 30**

**3 BALL PLAY**

**A-12522 – 3900, 5300, 6100**

**A-12809 – 4000, 5400, 6200**

**A-12523 – 4100, 5500, 6300**

**\* A-12524 – 4200, 5600, 6400**

**A-12810 – 4300, 5700, 6500**

**A-12525 – 4400, 5800, 6600**

**A-12811 – 4500, 5900, 6700**

**A-12817 – 10, 14, 17**

**A-12818 – 10, 15, 17**

**\* A-12819 – 11, 15, 17**

**A-12820 – 11, 16, 18**

**A-12821 – 12, 15, 17**

A-12806-1

290

A-12522

1 REPLAY FOR EACH  
 SCORE OF

3900 POINTS

5300 POINTS

6100 POINTS

A-12523

1 REPLAY FOR EACH  
 SCORE OF

4100 POINTS

5500 POINTS

6300 POINTS

A-12524

1 REPLAY FOR EACH  
 SCORE OF

4200 POINTS

5600 POINTS

6400 POINTS

A-12525

1 REPLAY FOR EACH  
 SCORE OF

4400 POINTS

5800 POINTS

6600 POINTS

A-12526

1 REPLAY FOR EACH  
 SCORE OF

5000 POINTS

6400 POINTS

7200 POINTS

A-12527

1 REPLAY FOR EACH  
 SCORE OF

5200 POINTS

6600 POINTS

7400 POINTS

A-12809

1 REPLAY FOR EACH  
 SCORE OF

4000 POINTS

5400 POINTS

6200 POINTS

A-12810

1 REPLAY FOR EACH  
 SCORE OF

4300 POINTS

5700 POINTS

6500 POINTS

A-12811

1 REPLAY FOR EACH  
 SCORE OF

4500 POINTS

5900 POINTS

6700 POINTS

A-12812

1 REPLAY FOR EACH  
 SCORE OF

4700 POINTS

6100 POINTS

6900 POINTS

A-12813

1 REPLAY FOR EACH  
 SCORE OF

4800 POINTS

6200 POINTS

7000 POINTS

A-12814

1 REPLAY FOR EACH  
 SCORE OF

4900 POINTS

6300 POINTS

7100 POINTS

A-12815

1 REPLAY FOR EACH  
 SCORE OF

5100 POINTS

6500 POINTS

7300 POINTS

A-12816

1 REPLAY FOR EACH  
 SCORE OF

5300 POINTS

6700 POINTS

7500 POINTS

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

10 RUNS

14 RUNS

17 RUNS

A-12817

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

10 RUNS

15 RUNS

17 RUNS

A-12818

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

11 RUNS

15 RUNS

17 RUNS

A-12819

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

11 RUNS

16 RUNS

18 RUNS

A-12820

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

12 RUNS

15 RUNS

17 RUNS

A-12821

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

16 RUNS

22 RUNS

28 RUNS

A-12822

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

17 RUNS

22 RUNS

28 RUNS

A-12823

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

18 RUNS

23 RUNS

29 RUNS

A-12824

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

19 RUNS

23 RUNS

28 RUNS

A-12825

1 REPLAY WHEN EACH OF  
THE FOLLOWING NUMBER  
OF RUNS ARE SCORED.

19 RUNS

24 RUNS

30 RUNS

A-12826

Font used: Futura XBlk BT, Futura Md BT, Futura Hv BT, News Gothic MT Std, Type Embellishments Two

**Cards status:**

B-12805 3 ball instruction card confirmed.

B-12805 5 ball instruction card needed to verify.

A-12806-1 index card confirmed.

All score cards according to the index card confirmed.

B-12831 post adjustment card is an original image.

A-9995 Ball-in-Play card confirmed. This card is being used behind the instruction card and  
is available on my website as A-9995 Back mask.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.