# BIG SHOT

**INSTRUCTIONS**

**ONE or TWO PLAYERS - 3 BALLS PER PLAYER**

## INSERT ONE COIN AND WAIT FOR MACHINE TO RESET BEFORE INSERTING COINS FOR SECOND PLAYER.

## PLAYERS TAKE TURNS SHOOTING AS SHOWN ON BACK GLASS.

## POINTS ARE SCORED AS INDICATED.

## BUMPER SCORES 1000 POINTS WHEN LIT.

## HITTING 1 THRU 8 OR 8 THRU 15 LIGHTS “SPECIAL WHEN LIT” ALTERNATELY.

## DROP TARGETS SCORE 500 POINTS.

## A TILT DOES NOT DISQUALIFY A PLAYER.

## MATCHING LAST TWO NUMBERS IN SCORE TO NUMBER THAT APPEARS ON BACK GLASS AFTER GAME IS OVER SCORES 1 REPLAY.

B-14708-1

343

# BIG SHOT

**INSTRUCTIONS**

**ONE or TWO PLAYERS - 5 BALLS PER PLAYER**

## INSERT ONE COIN AND WAIT FOR MACHINE TO RESET BEFORE INSERTING COINS FOR SECOND PLAYER.

## PLAYERS TAKE TURNS SHOOTING AS SHOWN ON BACK GLASS.

## POINTS ARE SCORED AS INDICATED.

## BUMPER SCORES 100 POINTS WHEN LIT.

## HITTING 1 THRU 8 OR 8 THRU 15 LIGHTS “SPECIAL WHEN LIT” ALTERNATELY.

## DROP TARGETS SCORE 500 POINTS.

## A TILT DOES NOT DISQUALIFY A PLAYER.

## MATCHING LAST TWO NUMBERS IN SCORE TO NUMBER THAT APPEARS ON BACK GLASS AFTER GAME IS OVER SCORES 1 REPLAY.

B-14708-1

343

ADJUSTMENT PLUG LOCATION

LIGHTBOX POINT SCORE ADJ. & 3-5 BALL ADJ.

BOTTOM PANEL 1ST COIN CHUTE ADJ. & 2ND

CHUTE ADJ.

A-13865 50,000 - 64,000 - 72,000

A-13959 53,000 - 67,000 - 75,000

A-13960 56,000 - 70,000 - 78,000

† A-14710 59,000 - 73,000 - 81,000

A-14308 62,000 - 76,000 - 84,000

✽ A-13868 65,000 - 79,000 - 87,000

A-14711 69,000 - 83,000 - 91,000

A-14712 74,000 - 88,000 - 96,000

A-13870 77,000 - 91,000 - 99,000

A-14474 81,000 - 95,000 - 99,000

A-14709-2

343

**SCORE CARDS ARE LISTED FROM LIBERAL TO**

**CONSERVATIVE.**

**RECOMMENDED CARDS ARE MARKED † FOR 3 BALL**

✽ **FOR 5 BALL.**



1 REPLAY FOR EACH SCORE OF 53,000 POINTS.

1 REPLAY FOR EACH SCORE OF 67,000 POINTS.

1 REPLAY FOR EACH SCORE OF 75,000 POINTS.

A-13959

1 REPLAY FOR EACH SCORE OF 50,000 POINTS.

1 REPLAY FOR EACH SCORE OF 64,000 POINTS.

1 REPLAY FOR EACH SCORE OF 72,000 POINTS.

A-13865

1 REPLAY FOR EACH SCORE OF 56000 POINTS.

1 REPLAY FOR EACH SCORE OF 70,000 POINTS.

1 REPLAY FOR EACH SCORE OF 78,000 POINTS.

A-13960

1 REPLAY FOR EACH SCORE OF 59,000 POINTS.

1 REPLAY FOR EACH SCORE OF 73,000 POINTS.

1 REPLAY FOR EACH SCORE OF 81,000 POINTS.

A-14710

1 REPLAY FOR EACH SCORE OF 62,000 POINTS.

1 REPLAY FOR EACH SCORE OF 76,000 POINTS.

1 REPLAY FOR EACH SCORE OF 84,000 POINTS.

A-14308

1 REPLAY FOR EACH SCORE OF 65,000 POINTS.

1 REPLAY FOR EACH SCORE OF 79,000 POINTS.

1 REPLAY FOR EACH SCORE OF 87,000 POINTS.

A-13868

1 REPLAY FOR EACH SCORE OF 77,000 POINTS.

1 REPLAY FOR EACH SCORE OF 91,000 POINTS.

1 REPLAY FOR EACH SCORE OF 99,000 POINTS.

A-13870

1 REPLAY FOR EACH SCORE OF 74,000 POINTS.

1 REPLAY FOR EACH SCORE OF 88,000 POINTS.

1 REPLAY FOR EACH SCORE OF 96,000 POINTS.

A-14712

1 REPLAY FOR EACH SCORE OF 69,000 POINTS.

1 REPLAY FOR EACH SCORE OF 83,000 POINTS.

1 REPLAY FOR EACH SCORE OF 91,000 POINTS.

A-14711

1 REPLAY FOR EACH SCORE OF 81,000 POINTS.

1 REPLAY FOR EACH SCORE OF 95,000 POINTS.

1 REPLAY FOR EACH SCORE OF 99,000 POINTS.

A-14474

**S**

START  
RELAY

**Q**

BALL RETURN  
CONTROL  
RELAY

**P**

ADD  
PLAYER  
UNIT RELAY

**W**

2nd CHUTE  
RELAY

**O**

BALL  
RETURN  
RELAY

**U**

CONTROL  
BANK RESET  
RELAY

Strip size: 226x25mm

**T**

TILT  
RELAY

**J**

BONUS SCORE  
CONTROL  
RELAY

**R**

HOLD  
RELAY

**I**

BONUS  
SCORE  
RELAY

**D**

500  
POINT  
RELAY

**H**

TILT  
HOLD  
RELAY

**C**

ADD  
BONUS  
UNIT RELAY

**V**

REPLAY  
BUTTON  
RELAY

Strip size: 218x25mm

HB

3000  
BONUS VALUE  
RELAY  
A-1118 COIL

**SB**2

RESET CONTROL  
SWITCHES  
NO COIL

**SB**1

RESET CONTROL  
RELAY  
A-1118 COIL

**XB**

LAST BALL  
RELAY  
A-1118 COIL

QB2

GAME OVER  
SWITCHES  
NO COIL

QB1

GAME OVER  
RELAY  
A-1118 COIL

ZB

1st PLAYER  
RELAY  
A-1118 COIL

PB

2nd PLAYER  
RELAY  
A-1118 COIL

LB

2000  
BONUS VALUE  
RELAY  
A-1118 COIL

Strip size: 273x17mm

**1ST COIN CHUTE**

**ADJUSTMENT**

**2ND CHUTE ADJ.**

**1 COIN - PLAY**

BANK SETUP

**CAUTION**

REPLACE ONLY WITH

10 AMP. SLO-BLO FUSE

**PRIMARY FUSE  
5 AMP. SLO-BLO**

**2ND CHUTE  
ADJUSTMENT**

**5 PLAYS**

**4 PLAYS**

**3 PLAYS**

**2 PLAYS**

Used fonts: Tremolo, Futura Hv BT, Futura LT condensed, Futura Md BT, News Gothic Std, Segoe UI Symbol,  
 AlternateGotNo3D, Helvetica,

**Cards status:**

B-14708-1 instruction cards confirmed.

A-14709-2 score index card confirmed.

All score card confirmed.

Relay strips confirmed.

Labels confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.