## BRITE STAR

SK389-8

143

## ONE OR TWO PLAYERS

## INSTRUCTIONS

## INSERT ONE COIN AND WAIT FOR MACHINE TO RESET BEFORE INSERTING COIN FOR SECOND PLAYER.

## PLAYERS TAKE TURNS SHOOTING AS SHOWN ON BACK GLASS.

## POINTS ARE SCORED AS INDICATED.

## HITTING STAR TARGET SCORES 10 POINTS AND LIGHTS 10 TIMES VALUE LIGHT.

## REPLAYS NEED NOT BE PLAYED OFF BEFORE INSERTING NEXT COIN.

## A TILT BY ONE PLAYER DISQUALIFIES ONLY THAT PLAYER.

SK389-1

143

## SK389-2 SCORE CARD RECOMMENDED

## FOR 3 BALL PLAY.

## SK359-9 SCORE CARD RECOMMENDED

## FOR 5 BALL PLAY.

SK389-7

143

## 1 REPLAY FOR EACH SCORE OF 600 POINTS.

## 1 REPLAY FOR EACH SCORE OF 900 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1000 POINTS.

SK389-2

143

## 1 REPLAY FOR EACH SCORE OF 1200 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1400 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1500 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1600 POINTS.

SK389-3

143

## 1 REPLAY FOR EACH SCORE OF 1300 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1500 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1600 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1700 POINTS.

SK389-4

143

## 1 REPLAY FOR EACH SCORE OF 1300 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1500 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1700 POINTS.

SK389-6

143

## 1 REPLAY FOR EACH SCORE OF 1200 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1400 POINTS.

## 1 REPLAY FOR EACH SCORE OF 1600 POINTS.

SK359-9

132

## MATCHING LAST NUMBER IN SCORE TO NUMBER THAT APPEARS ON BACK GLASS WHEN GAME IS OVER AWARDS 1 REPLAY.

## MATCHING LAST NUMBER IN BOTH SCORES TO NUMBER THAT APPEARS ON BACK GLASS WHEN GAME IS OVER AWARDS 10 REPLAYS. (5 FOR EACH PLAYER).

SK329-10

## MATCHING LAST NUMBER IN SCORE TO NUMBER THAT APPEARS ON BACK GLASS WHEN GAME IS OVER AWARDS 1 REPLAY.

SK329-11

Strip size: 333x17mm

4B

2ND PLAYER

THOUSANDS RELAY

A-1118

COIL

3B

1ST PLAYER

THOUSANDS RELAY

A-1118

COIL

SK389-10

2B

2ND PLAYER

MATCH RELAY

A-1118

COIL

1B

1ST PLAYER

MATCH RELAY

A-1118

COIL

TB1

1ST PLAYER

TILT RELAY

A-1118

COIL

TB2

2ND PLAYER

TILT RELAY

A-1118

COIL

143

TB2

2ND PLAYER

TILT RELAY

A-1118

COIL

PB

2ND PLAYER

RELAY

A-1118

COIL

ZB

1ST BALL

RELAY

A-1118

COIL

QB

GAME OVER

RELAY

A-1118

COIL

SB

START

RELAY

A-1118

COIL

XB

LAST BALL

RELAY

A-1118

COIL

**C A U T I O N**

REPLACE ONLY WITH

1 AMP. SLO-BLO FUSE

SK381

**3**

**5**

BALLS PER

PLAYER ADJ.

SK302-4

ON

143

STAR

LIGHT

ADJUSTMENT

SK389-44

OFF

SK370-15

PLAYBOARD

LIGHT FUSE

LIGHTBOX

LIGHT FUSE

25 VOLT  
 FUSE

MATCH  
FEATURE

IN OUT

SK339-16

25 CENT

CHUTE

ADJUSTMENT

10 REPLAYS

2 REPLAYS

5 PLAYS

4 PLAYS

3 PLAYS

DOUBLE

MATCH

FEATURE

(THESE PLUGS ARE LOCATED ON THE BOTTOM PANEL.)

POINT SCORE ADJ.

3

BALL

3

BALL

5

BALL

5

BALL

SK367-13

135

1500

1400

1300

1200

1100

500

400

300

200

100

1000

900

800

700

600

1000

1900

1800

1700

1600

Used fonts: Eden Bold, Futura Hv BT, Futura Md BT, Tremolo, Helvetica

Card size: 154x36mm, 154x108mm, 154x58mm

**Cards status:**

SK389-8 title card confirmed.

SK389-1 instruction card confirmed.

SK389-7 recommended score card confirmed.

SK389-2 score card confirmed.

SK389-3 score card confirmed.

SK389-4 score card confirmed.

SK389-6 score card confirmed.

SK359-5 score card confirmed.

SK329-10 generic match card confirmed.

SK329-11 generic match card confirmed.

SK389-10 relay strip confirmed.

SK381 fuse label confirmed.

SK302-4 balls per player adj. confirmed.

SK389-44 Star Light adjustment label confirmed.

SK370-15 fuse label confirmed.

SK339-16 bottom panel plugs confirmed.

SK367-13 Point Score Adjustment confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.