**ADJUSTMENT OF COIN SWITCH FOR 10 CENTS PLAY**

1. **REPLACE SWITCH ARM A-4401 (25¢) WITH A-4400 (10¢) ENCLOSED IN  
   THE INSTRUCTIONS ENVELOPE.**
2. **ADJUST SPACING BETWEEN POINTS TO .018.**
3. **ADJUST PRESSURE OF LONG BLADE AGAINST POINT OF CONTACT WITH  
   WIRE FORM TO 5 GRAMS.**
4. **ADJUST PRESSURE OF SHORT BLADE AGAINST POINT OF CONTACT TO 2  
   GRAMS. (MEASURED AT END OF BLADE.)**

**THE TOTAL PRESSURE WITH SWITCH CLOSED MEASURED AT POINT OF  
CONTACT TO WIRE FORM AND INCLUDING .015 OVER TRAVEL (MAKE)  
SHOULD BE 9 GRAMS.**

A-13354

Fonts used: News Gothic Std

**Cards status:**

A-13354 card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.