
MOTOR SWITCH POSITIONS

MOTOR 3½ B - BRAKE



#

3½

MOTOR 4B SW. – EXTRA CHUTE COUNT.

INSIDE SW. – EXTRA CHUTE COUNT.

MOTOR 4C SECOND SW. – OPENS CIRCUIT TO 0-9 UNIT.

(S-Position) THIRD SW. – SCORING.

FOURTH SW. – BANK RESET.

4

#

#

3

MOTOR 3B – SW – SCORING.

INSIDE SW. – EXTRA CHUTE COUNT – RESETS  
MOTOR 1A ONES, TENS & HUNDREDS UNIT.

(S-Position) SECOND SW. – SCORING.

THIRD SW. – TRIPS “X” RELAY.

MOTOR 1B SW. – SCORING.

INSIDE SW. – MOTOR RUNOUT.

MOTOR 1C SECOND SW. – OPENS CIRCUIT TO PLAYBOARD  
 (S-Position) CONTACTS & MATCH DELAY.

THIRD SW. – OPENS CIRCUIT TO REPLAY BUTTON.

MOTOR 1D SW. – SAME VALUE SPECIAL SWITCH.

INSIDE SW. – OPENS “G”, “U” & “V” RELAY.

MOTOR 2B LOCKINS.

SECOND SW. – OPENS “W” RELAY LOCKIN.

THIRD SW. – ACTUATES “Z” RELAY.

INSIDE SW. – SCORING.

SECOND SW. – EXTRA CHUTE COUNT.

MOTOR 2C THIRD SW. – SUBTRACT REPLAY, ADD TOTAL  
 (L-Position) PLAY METER.

FOURTH SW. – COMPLETES CIRCUIT TO “X”


RELAY, SCORES REPLAY ON  
 MATCH.

2

#

1

#



E

D

C

B


A

*S L*

C-9646 229

MOTOR SWITCH POSITIONS

MOTOR 3½ B - BRAKE



#

3½

INSIDE SW. – OPENS CIRCUIT TO 0-9 UNIT.

MOTOR 4C SECOND SW. – SCORING.

(S-Position) THIRD SW. – BANK RESET.

4

#

#

3

INSIDE SW. – RESETS ONES, TENS & HUNDREDS  
MOTOR 1A UNIT.

(S-Position) SECOND SW. – SCORING.

THIRD SW. – TRIPS “X” RELAY.

MOTOR 1B SW. – SCORING.

INSIDE SW. – MOTOR RUNOUT.

MOTOR 1C SECOND SW. – OPENS CIRCUIT TO PLAYBOARD  
 (S-Position) CONTACTS & MATCH DELAY.

THIRD SW. – OPENS CIRCUIT TO REPLAY BUTTON.

MOTOR 1D SW. – SAME VALUE SPECIAL SWITCH.

MOTOR 3B – SW – SCORING.

INSIDE SW. – OPENS “G”, “W” & “V” RELAY.

MOTOR 2B LOCKINS.

SECOND SW. – ACTUATES “Z” RELAY.

INSIDE SW. – SCORING.

SECOND SW. – SUBTRACT REPLAY, ADD TOTAL  
MOTOR 2C PLAY METER.

(L-Position) THIRD SW. – COMPLETES CIRCUIT TO “X”


RELAY, SCORES REPLAY ON MATCH.

2

#

1

#



E

D

C

B

A

*S L*

C-9646 229

Font used: Futura Hv BT, Futura Md BT

Size:102x203mm

**Cards status:**

C-9646 Motor Switch Positions card (black) confirmed.

C-9646 Motor Switch Positions card (red) confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.