## THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED TRANSFORMER TO MAINTAIN THE USUAL FINE FLIP- PER ACTION AT LOW VOLTAGE. MOVING THE RED WITH YELLOW TRACER WIRE ON THE TRANSFORMER FROM THE NORMAL TAP TO THE HIGH TAP ALLOWS THE MACHINE TO OPERATE AT A REDUCED VOLTAGE. IN NO CASE SHOULD THE RED WITH YELLOW TRACER WIRE BE LEFT ON THE HIGH TAP WHEN THE LOCA- TION VOLTAGE EQUALS OR EXCEEDS 110 VOLTS.

SK382-6

## THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED TRANSFORMER TO MAINTAIN THE USUAL FINE FLIPPER ACTION AT LOW VOLTAGE. MOVING THE RED WITH YELLOW TRACER WIRE ON THE TRANSFORMER FROM THE NORMAL TAP TO THE HIGH TAP ALLOWS THE MACHINE TO OPERATE AT A REDUCED VOLTAGE. IN NO CASE SHOULD THE RED WITH YELLOW TRACER WIRE BE LEFT ON THE HIGH TAP WHEN THE LOCATION VOLTAGE EQUALS OR EXCEEDS 110 VOLTS.

SK382-6

Used fonts: Futura Md BT

Card size: 114x67mm (black text), 108x54mm (red text)

**Cards status:**

SK382-6 transformer card confirmed.

Originally this card is from Gottlieb - Falstaff.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.