**D**

500

POINT

RELAY

**S**

START

RELAY

**Q**

BALL RETURN  
CONTROL

RELAY

**P**

ADD  
PLAYER  
UNIT RELAY

**W**

2nd  
CHUTE

RELAY

**O**

BALL

RETURN

RELAY

**U**

CONTROL

BANK RESET

RELAY

**I**

BONUS

SCORE

RELAY

**DX**

MOTOR

ID

RELAY

**J**

BONUS

SCORE

CONTROL

RELAY

**R**

HOLD

RELAY

**H**

TILT

HOLD

RELAY

**C**

ADD

BONUS

UNIT RELAY

**T**

TILT

RELAY

**V**

REPLAY

BUTTON

RELAY

**HB**

3000

BONUS VALUE

RELAY

A-1118 COIL

**PB**4

4th

PLAYER

RELAY

A-1118 COIL

**PB**3

3rd

PLAYER

RELAY

A-1118 COIL

**PB**2

2nd

PLAYER

RELAY

A-1118 COIL

**LB**

2000

BONUS VALUE

RELAY

A-1118 COIL

**SB**2

RESET

CONTROL

SWITCHES

NO COIL

**SB**1

RESET

CONTROL

RELAY

A-1118 COIL

**XB**

LAST

BALL

RELAY

A-1118 COIL

**QB**2

GAME

OVER

SWITCHES

NO COIL

**QB**1

GAME

OVER

RELAY

A-1118 COIL

**ZB**

1st

BALL

RELAY

A-1118 COIL

PRIMARY FUSE

5 AMP. SLO-BLO

**BANK SETUP**

**CAUTION**

**REPLACE ONLY WITH**

**10 AMP. SLO-BLO FUSE**

**POINT SCORE  
ADJUSTMENT**

A-13546

**(PLUGS)**

**0 (0)**

**10,000 (1)**

**20,000 (2)**

**30,000 (3)**

**40,000 (4)**

**50,000 (5)**

**60,000 (6)**

**70,000 (7)**

**80,000 (8)**

**90,000 (9)**

**NOTE: PLUG VALUE PLUG SOCKET VALUE EQUALS  
 POINT SCORE**

**(SOCKET)**

**4000 9000**

**3000 8000**

**2000 7000**

**1000 6000**

**10000 5000**

2ND CHUTE ADJ.

**5 PLAYS**

**4 PLAYS**

**3 PLAYS**

**2 PLAYS**

**1st COIN CHUTE**

**ADJUSTMENT**

**2nd CHUTE ADJ.**

**1 - PLAY**

Font used: HelvCondensed Normal, Helvetica, Futura BdCn BT, Futura Md BT.

**Cards status:**

Relay strip card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via Paypal.