## THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED TRANSFORMER TO MAINTAIN THE USUAL FINE FLIPPER ACTION AT LOW VOLTAGE. MOVING THE RED WIRE ON THE TRANSFORMER FROM THE NORMAL TAP TO THE HIGH TAP ALLOWS THE MACHINE TO OPERATE AT A REDUCED VOLTAGE. IN NO CASE SHOULD THE RED WIRE BE LEFT ON THE HIGH TAP WHEN THE LOCATION VOLTAGE EQUALS OR EXCEEDS 110 VOLTS.

## SK91-10

Used fonts: Futura Md BT

**Cards status:**

SK91-10 Transformer card confirmed. (115x90mm).

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.