**INSTRUCTIONS**

**ONE or TWO PLAYERS – 3 BALLS PER PLAYER**

INSERT ONE COIN AND WAIT FOR MACHINE TO RESET BEFORE INSERTING  
 COIN FOR SECOND PLAYER.

PLAYERS TAKE TURNS SHOOTING AS SHOWN ON BACK GLASS.

POINTS ARE SCORED AS INDICATED.

1 ADVANCE IS REGISTERED FOR EACH 10 POINTS AND 5 ADVANCES  
 ARE REGISTERED FOR EACH 50 POINTS.

ROLLUNDER TARGET SCORES 10 POINTS FOR EACH REVOLUTION.

EVERY 10 ADVANCES SCORES 1 LAP.

LAP VALUE IS SCORED UPON COMPLETION OF BALL IN PLAY.

LAP VALUE IS 50 POINTS UNLESS OTHERWISE NOTED.

A TILT DOES NOT DISQUALIFY A PLAYER.

MATCHING LAST NUMBER IN SCORE TO NUMBER THAT APPEARS  
 ON BACK GLASS AFTER GAME IS OVER SCORES 1 REPLAY.

BALL IN PLAY

291

B-13006-1

**INSTRUCTIONS**

**ONE or TWO PLAYERS – 5 BALLS PER PLAYER**

INSERT ONE COIN AND WAIT FOR MACHINE TO RESET BEFORE INSERTING  
 COIN FOR SECOND PLAYER.

PLAYERS TAKE TURNS SHOOTING AS SHOWN ON BACK GLASS.

POINTS ARE SCORED AS INDICATED.

1 ADVANCE IS REGISTERED FOR EACH 10 POINTS AND 5 ADVANCES  
 ARE REGISTERED FOR EACH 50 POINTS.

ROLLUNDER TARGET SCORES 10 POINTS FOR EACH REVOLUTION.

EVERY 10 ADVANCES SCORES 1 LAP.

LAP VALUE IS SCORED UPON COMPLETION OF BALL IN PLAY.

LAP VALUE IS 50 POINTS UNLESS OTHERWISE NOTED.

A TILT DOES NOT DISQUALIFY A PLAYER.

MATCHING LAST NUMBER IN SCORE TO NUMBER THAT APPEARS  
 ON BACK GLASS AFTER GAME IS OVER SCORES 1 REPLAY.

BALL IN PLAY

291

B-13006-1

**SCORE CARDS ARE LISTED FROM LIBERAL TO CONSERVATIVE.**

**CARDS MARKED \* ARE RECOMMENDED FOR FEATURE ADJ. IN  
CONSERVATIVE.**

**CARDS MARKED + ARE RECOMMENDED FOR FEATURE ADJ. IN LIBERAL.**

**ADJUSTMENT PLUG LOCATION**

**INSIDE LIGHTBOX** ! **POINT SCORE ADJ., 3-5 BALL ADJ.  
AND FEATURE ADJ.**

**BOTTOM PANEL** ! **1st & 2nd CHUTE ADJ. AND 3rd CHUTE ADJ.**

**5 BALL PLAY**

**A-12847 (3000, 4400, 5200)**

**A-12699 (3400, 4800, 5600)**

**\* A-12496 (3800, 5200, 6000)**

**A-12848 (4200, 5600, 6400)**

**+ A-12701 (4500, 5900, 6700)**

**A-12498 (4800, 6200, 7000)**

**A-12499 (5100, 6500, 7300)**

**3 BALL PLAY**

**A-13009 (2200, 3600, 4400)**

**A-12697 (2600, 4000, 4800)**

**\* A-12847 (3000, 4400, 5200)**

**+ A-12699 (3400, 4800, 5600)**

**A-12496 (3800, 5200, 6000)**

**A-12848 (4200, 5600, 6400)**

**A-12701 (4500, 5900, 6700)**

A-13686

292

1 REPLAY FOR EACH SCORE OF 2200 POINTS.

1 REPLAY FOR EACH SCORE OF 3600 POINTS.

1 REPLAY FOR EACH SCORE OF 4400 POINTS.

A-13009

1 REPLAY FOR EACH SCORE OF 2600 POINTS.

1 REPLAY FOR EACH SCORE OF 4000 POINTS.

1 REPLAY FOR EACH SCORE OF 4800 POINTS.

A-12697

1 REPLAY FOR EACH SCORE OF 3000 POINTS.

1 REPLAY FOR EACH SCORE OF 4400 POINTS.

1 REPLAY FOR EACH SCORE OF 5200 POINTS.

A-12847

1 REPLAY FOR EACH SCORE OF 3400 POINTS.

1 REPLAY FOR EACH SCORE OF 4800 POINTS.

1 REPLAY FOR EACH SCORE OF 5600 POINTS.

A-12699

1 REPLAY FOR EACH SCORE OF 3800 POINTS.

1 REPLAY FOR EACH SCORE OF 5200 POINTS.

1 REPLAY FOR EACH SCORE OF 6000 POINTS.

A-12496

1 REPLAY FOR EACH SCORE OF 4200 POINTS.

1 REPLAY FOR EACH SCORE OF 5600 POINTS.

1 REPLAY FOR EACH SCORE OF 6400 POINTS.

A-12848

1 REPLAY FOR EACH SCORE OF 4500 POINTS.

1 REPLAY FOR EACH SCORE OF 5900 POINTS.

1 REPLAY FOR EACH SCORE OF 6700 POINTS.

A-12701

1 REPLAY FOR EACH SCORE OF 4800 POINTS.

1 REPLAY FOR EACH SCORE OF 6200 POINTS.

1 REPLAY FOR EACH SCORE OF 7000 POINTS.

A-12498

1 REPLAY FOR EACH SCORE OF 5100 POINTS.

1 REPLAY FOR EACH SCORE OF 6500 POINTS.

1 REPLAY FOR EACH SCORE OF 7300 POINTS.

A-12499

Font used: Futura XBlk BT, Futura Md BT, Futura Hv BT, News Gothic MT Std, Type Embellishments Two

**Cards status:**

B-13006-1 3&5 ball instruction card confirmed.

A-13686 index card (Snow Queen) confirmed.

All listed score cards confirmed.

A-9995 Ball-in-Play card confirmed. This card is being used behind the instruction card and   
is available on my website as A-9995 Back mask.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.