THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED  
TRANSFORMER TO MAINTAIN THE USUAL FINE FLIP-  
PER ACTION AT LOW VOLTAGE. MOVING THE RED  
WITH YELLOW TRACER WIRE ON THE TRANSFORMER  
FROM THE NORMAL TAP TO THE HIGH TAP ALLOWS  
THE MACHINE TO OPERATE AT A REDUCED VOLTAGE.  
IN NO CASE SHOULD THE RED WITH YELLOW TRACER  
WIRE BE LEFT ON THE HIGH TAP WHEN THE LOCA-  
TION VOLTAGE EQUALS OR EXCEEDS 110 VOLTS.

A-6279

THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED  
TRANSFORMER TO MAINTAIN THE USUAL FINE  
FLIPPER ACTION AT LOW VOLTAGE. MOVING  
THE RED WIRE ON THE TRANSFORMER FROM THE  
NORMAL TAP TO THE HIGH TAP ALLOWS THE  
MACHINE TO OPERATE AT A REDUCED VOLTAGE.  
IN NO CASE SHOULD THE RED WIRE BE LEFT ON  
THE HIGH TAP WHEN THE LOCATION VOLTAGE  
IS NORMAL.

A-6423-2

THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED  
TRANSFORMER TO MAINTAIN THE USUAL FINE  
FLIPPER ACTION AT LOW VOLTAGE. MOVING  
THE RED WIRE ON THE TRANSFORMER FROM THE  
NORMAL TAP TO THE HIGH TAP ALLOWS THE  
MACHINE TO OPERATE AT A REDUCED VOLTAGE.  
IN NO CASE SHOULD THE RED WIRE BE LEFT ON  
THE HIGH TAP WHEN THE LOCATION VOLTAGE  
IS NORMAL.

A-6423-2

Font used: Futura Md BT, HelveticaNeueLT Std Med.

Card size: 114x63mm

**Cards status:**

A-6279 Special Transformer card confirmed.

A-6423-2 Special Transformer card both versions confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.