THIS GAME IS EQUIPPED WITH A SPECIAL TAPPED  
TRANSFORMER TO MAINTAIN THE USUAL FINE PLAYBOARD  
ACTION AT LOW VOLTAGE. MOVING THE WIRE ON THE  
TRANSFORMER FROM THE NORMAL TAP TO THE HIGH TAP  
ALLOWS THE MACHINE TO OPERATE AT A REDUCED  
VOLTAGE. IN NO CASE SHOULD THE HIGH TAP BE USED  
WHEN THE LOCATION VOLTAGE IS NORMAL.

A-19073

Font used: HelveticaNeueLT Std Med.

**Cards status:**

A-19073 Special Transformer card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.