**LINE VOLTAGE**

BANK SETUP  
CAUTION  
REPLACE ONLY WITH  
½ AMP. SLO-BLO FUSE

BANK SETUP  
CAUTION  
REPLACE ONLY WITH  
½ AMP. SLO-BLO FUSE

CREDIT  
CONTROL RELAY

BANK SETUP  
CAUTION  
REPLACE ONLY WITH  
1 AMP. SLO-BLO FUSE

BANK SETUP  
CAUTION  
REPLACE ONLY WITH  
1 AMP. SLO-BLO FUSE

2 COINS PER  
PLAY RELAY

2 COINS

3 PLAYS

COIN CHUTE ADJUSTMENT

**A-17391**

1 COIN

2 PLAYS

1 COIN

1 PLAY

**PRIMARY FUSE  
5 AMP. SLO-BLO**

**TILT** **RESET**

**ADJUSTMENT**

**IN**

**OUT**

A-9609

25

VOLT

FUSE

12

AMP.

PLAYBOARD

LIGHT

FUSE

12

AMP.

LIGHTBOX

LIGHT

FUSE

10

AMP.

C

LEFT TARGET  
BANK SEQ.  
RELAY

O

BALL  
RETURN  
RELAY

D

RIGHT TARGET  
BANK SEQ.  
RELAY

S

START  
RELAY

E

500  
POINT  
RELAY

H

TILT  
HOLD  
RELAY

F

5000 POINT OR  
SEQUENCE BANK  
RESET RELAY

R

HOLD  
RELAY

G

WOW AND  
TARGET BANK  
RESET RELAY

T

TILT  
RELAY

U

5000 POINT &  
TARGET BANK  
RESET RELAY

Q

SERIES  
RELAY

NOTE: PLUG VALUE PLUS SOCKET VALUE EQUALS HIGH SCORE.

HIGH SCORE ADJUSTMENT

0 (0) 100,000 (1)

40,000 90,000

30,000 80,000

20,000 70,000

10,000 60,000

0 50,000

A-14426-1

Font used: Franklin Gothic Medium Cond, AlternateGotNo3D,  
 Futura Hv BT, Futura Md BT, Futura XBlk BT,

All labels confirmed.

If you have any information about these labels, please let me know.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.