Be Sure To Insert All Lightbox Plugs Before  
Attaching Cord To 115 V. Line. Do Not  
Make Any Adjustments On Contacts Or  
Step Switches While Machine Is Connected  
To 115 V. Line.

A-6235-1

VERY IMPORTANT

VERY IMPORTANT

A-6235-2

INSERT ALL LIGHTBOX PLUGS IN THE PROPER

SOCKETS BEFORE PLUGGING IN THE LINE CORD.

DISCONNECT THE LINE CORD BEFORE MAKING

ADJUSTMENTS TO CONTACTS OR UNITS.

A-6235-2

VERY IMPORTANT

INSERT **ALL** LIGHTBOX PLUGS IN THE PROPER  
SOCKETS **BEFORE** PLUGGING IN THE LINE CORD.  
  
DISCONNECT THE LINE CORD BEFORE MAKING  
ADJUSTMENTS TO CONTACTS OR UNITS.

Be Sure To Insert All Lightbox Plugs Before  
Attaching Cord To 110 V. Line. Do Not  
Make Any Adjustments On Contacts Or Step  
Switches While Machine Is Connected To  
110 V. Line.

SK-64-1

VERY IMPORTANT

Font used: FranklinGothicEF, Futura Md BT, HelveticaNeueLT Std Med, HelveticaNeueLT Std Med Cn,  
 Futura BdCn BT.

**Cards status:**

A-6235-1 Very Important card confirmed.

A-6235-2 Very Important card confirmed.

A-6235-2 Very Important card second version confirmed.

SK64-1 Very Important card confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.