# VOLLEY

**INSTRUCTIONS**

**3 BALLS PER PLAY**

## INSERT COIN OR PRESS CREDIT BUTTON TO RESET MACHINE.

## BLUE AND GREEN BUMPERS SCORE 100 POINTS OR 1000 POINTS WHEN LIT.

**COMPLETING BLUE, YELLOW AND GREEN DROP TARGETS LIGHT TOP  
ROLLOVERS FOR SPECIAL.**

**SPECIAL SCORES ONE REPLAY.**

**BOTTOM CONTACTS SCORE 1000 POINTS.**

**MATCHING LAST TWO NUMBERS IN SCORE TO NUMBER THAT APPEARS  
ON BACK GLASS AFTER GAME IS OVER SCORES ONE REPLAY.**

**394**

**B-16681-1**

# VOLLEY

**INSTRUCTIONS**

**5 BALLS PER PLAY**

## INSERT COIN OR PRESS CREDIT BUTTON TO RESET MACHINE.

## BLUE AND GREEN BUMPERS SCORE 10 POINTS OR 100 POINTS WHEN LIT.

**COMPLETING BLUE, YELLOW AND GREEN DROP TARGETS LIGHT TOP  
ROLLOVERS ALTERNATELY FOR SPECIAL.**

**SPECIAL SCORES ONE REPLAY.**

**BOTTOM CONTACTS SCORE 100 POINTS.**

**MATCHING LAST TWO NUMBERS IN SCORE TO NUMBER THAT APPEARS  
ON BACK GLASS AFTER GAME IS OVER SCORES ONE REPLAY.**

**394**

**B-16681-1**

**SCORE CARDS ARE LISTED FROM LIBERAL**

**TO CONSERVATIVE. RECOMMENDED**

**CARDS ARE MARKED.**

**✽ FOR 3 BALL † FOR 5 BALL.**

A-17111 90,000 - 120,000 - 150,000

A-17112 100,000 - 120,000 - 160,000

✽ A-17113 100,000 - 140,000 - 160,000

A-17114 110,000 - 140,000 - 160,000

A-17115 120,000 - 140,000 - 160,000

A-16608 120,000 - 150,000 - 170,000

† A-17116 130,000 - 150,000 - 170,000

A-16610 130,000 - 150,000 - 180,000

A-16611 130,000 - 160,000 - 180,000

A-16613 140,000 - 170,000 - 190,000

ADJUSTMENT PLUG LOCATION.

PLAYBOARD 3-5 BALL ADJ.

LIGHT BOX POINT SCORE ADJ.

BOTTOM PANEL 1st & 2nd CHUTE ADJ., “W” RELAY

ADJ.







394

A-16683-2

1 REPLAY FOR EACH SCORE OF 90,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 120,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

A-17111

1 REPLAY FOR EACH SCORE OF 100,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 120,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-17112

1 REPLAY FOR EACH SCORE OF 100,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 140,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-17113

1 REPLAY FOR EACH SCORE OF 110,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 140,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 160,000 POINTS.

A-17114

1 REPLAY FOR EACH SCORE OF 120,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 140,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 150,000 POINTS.

A-17115

1 REPLAY FOR EACH SCORE OF 120,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 150,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 170,000 POINTS.

A-16608

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 150,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 170,000 POINTS.

A-17116

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 150,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 180,000 POINTS.

A-16610

1 REPLAY FOR EACH SCORE OF 130,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 160,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 180,000 POINTS.

A-16611

1 REPLAY FOR EACH SCORE OF 140,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 170,000 POINTS.  
1 REPLAY FOR EACH SCORE OF 190,000 POINTS.

A-16613

1 REPLAY FOR EACH SCORE OF POINTS.  
1 REPLAY FOR EACH SCORE OF POINTS.  
1 REPLAY FOR EACH SCORE OF POINTS.

A-12689-1

1 REPLAY FOR EACH SCORE OF POINTS.  
1 REPLAY FOR EACH SCORE OF POINTS.

A-16141

PRIMARY FUSE

5 AMP. SLO-BLO

**“W” RELAY  
ADJUSTMENT**

**3 5**

**3-5 BALL  
ADJUSTMENT**

**1ST AND 2ND  
CHUTE ADJUSTMENT**



**5**

**4**

**3**

**2**

**1 COIN**

**1 PLAY**

**1 COIN**

**ADJ.**

**2, 3, 4 OR 5**

**PLAYS**

**BANK SETUP**

**CAUTION**

**REPLACE ONLY WITH**

**2 AMP. SLO-BLO FUSE**



**1st CHUTE**

**2nd CHUTE**

**A-6231**

**A-16993**

LINE VOLTAGE

Font used: HelvCondensed Normal, Helvetica, Futura BdCn BT, Futura Md BT, Futura MdCn BT,

Futura Bk BT, Futura Std Medium, Futura Hv BT, Futura LT CondensedExtraBold, News Gothic Std

Card size: 154x108mm (instructions), 154x57mm (score)

**Cards status:**

B-16681-1 3 & 5 balls instruction card confirmed.

A-16683-2 index card confirmed

All score cards confirmed.

Relay strip confirmed, Fuse strip confirmed, Primary Fuse label confirmed, Bank Setup label confirmed, Line Voltage label confirmed.

W Relay Adjustment A-6231 confirmed.

Coin Chute Adjustment A-16993 confirmed.

3 & 5 ball Adjustment label confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.

**V**

ADD

REPLAY UNIT

RELAY

**H**

TILT

HOLD

RELAY

**U**

SPECIAL  
CONTROL

RELAY

**S**

START

RELAY

**Q**

TARGET  
BANK RESET  
RELAY

**W**

2nd  
CHUTE

RELAY

**G**

5000

POINT

RELAY

**O**

BALL

RETURN

RELAY

**E**

500

POINT

RELAY

Connect to V

**T**

TILT

RELAY

**R**

HOLD

RELAY

25  
VOLT  
FUSE  
**10**  
AMP.

PLAYBOARD  
LIGHT  
FUSE  
**7½**  
AMP.

LIGHTBOX  
LIGHT  
FUSE  
**10**  
AMP.