1. Locate Switches S1 Thru S32 On MPU Assembly.
2. Set Switches For Desired Game Conditions.
3. Turn Game Off, Then On. Adjustments Are Then Complete.

**Switch Game**

**Game Adjustments Switch No. Function Function**

SPECIAL LITE AWARD S31 & S32 ON-ON FREE BALL & FREE GAME

S31 & S32 OFF-OFF 100,000 PTS.

S31 ON

S32 OFF FREE BALL

S31 OFF FREE GAME

S32 ON

EXTRA BALL ALTERNATION S27 OFF CONSTANT ON

ON ALTERNATE

OUTLANE SPECIAL S26 OFF OPEN ENDED

ON 1 SPECIAL

TARGET SPECIAL S25 OFF OPEN ENDED

ON 1 SPECIAL

OUTLANE SPECIAL S24 OFF 2nd TARGET RESET

ON 3rd TARGET RESET

EXTRA BALL S23 OFF BYPASS

ON AWARD

S-32

S-25

S-24

S-17

S-16

S-9

S-8

S-1

ON OFF

12C-266-3

Font used: Helvetica, CentSchbook Mono BT.

12C-266-3 (size 214 x 118 mm) confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.