**SWITCH**

**SYMBOL**

**SWITCH IDENTIFICATION**

**SWITCH**

**NO.**

**15**

**SOLENOID IDENTIFICATION**

**I.D. TRANS. WIRE**

**NO. NO. JACK COLOR DESCRIPTION**

**1 Q1 J2-9 G-O LEFT SLINGSHOT**

**2 Q2 J2-4 G-BLU RIGHT SLINGSHOT**

**3 Q3 . . . J2-5 G-B KNOCKER**

**4 Q4 J1-5 B-BLU OUTHOLE**

**5 Q5 J2-10 G-Y RIGHT DROP BANK**

**6 Q6 . . . J2-11 G-R TOP DROP BANK**

**7 Q7 J2-12 R-Y POP BUMPER**

**8 Q8 J5-10 B-O LEFT LANE KICK-OUT HOLE**

**9 Q9 . . . J5-9 R-BLU DROP TARGET #5**

**10 Q10 J5-15 O-W DROP TARGET #4**

**11 Q11 J5-14 O-B DROP TARGET #2**

**12 Q12 . . J5-13 O-G DROP TARGET #3**

**13 Q13 J5-12 B-Y DROP TARGET #7**

**14 Q14 J5-11 B-G DROP TARGET #6**

**15 Q15 J3-5 Y-W FLIPPER ENABLE RELAY**

**16 Q16 . . J5-8 G-W DROP TARGET #1**

**17 Q17 J5-7 O-R LEFT DROP BANK RESET**

**18 Q18 J5-3 R-W LOOP DROP TARGET**

**19 Q19 J2-8 Y-W COIN LOCK OUT**

**SWS. #1, 2, & 3 NO DIODE  
ALL OTHER SWITCH USE**

**DIODE 1N4004**

 **SYMBOL IF  
 .05 CAP IS  
 USED**

**R-Y (J3-2)**

**W-R (J2-1)**

**BRN-W (J2-2)**

**SWITCH WIRE JACK**

**NO. COLOR NO. DESCRIPTION**

**1 BLU J3-9 CHUTE (LEFT)**

**2 BRN-W J3-10 CHUTE (CENTER)**

**3 R-W J3-11 CHUTE (RIGHT)**

**4**  **W-B J2-11 LOOP ROLL UNDER**

**5 W-G J2-12 SPINNER**

**6 BLU-W J3-14 CREDIT (START) BUTTON**

**7 BLU-O J3-15 TILT**

**8 -Y- J2-15 SLAM**

**9 BRN J2-8 DROP TARGET #1**

**10 GREY J2-9 DROP TARGET #2**

**11 W-O J2-10 DROP TARGET #3**

**12 W-B J2-11 DROP TARGET #4**

**13 W-G J2-12 DROP TARGET #5**

**14 W-BRN J2-13 DROP TARGET #6**

**15 BRN-Y J2-14 DROP TARGET #7**

**16 -O- J2-15 DROP TARGET #8**

**17**  **BRN J2-8 TOP DEAD BUMPER**

**18 GREY J2-9 TOP 3 BANK LEFT TARGET**

**19 W-O J2-10 TOP 3 BANK MIDDLE TARGET**

**20 W-B J2-11 TOP 3 BANK RIGHT TARGET**

**21 W-G J2-12 LOOP DROP TARGET**

**22 W-BRN J2-13 RIGHT 3 BANK TOP TARGET**

**23 BRN-Y J2-14 RIGHT 3 BANK MIDDLE TARGET**

**24 -O- J2-15 RIGHT 3 BANK BOTTOM TARGET**

**25 BRN J2-8 RIGHT OUTLANE**

**26 GREY J2-9 LEFT OUTLANE**

**27 W-O J2-10 RIGHT RETURN LANE**

**28 W-B J2-11 LEFT RETURN LANE**

**29 W-G J2-12 RIGHT SLINGSHOT**

**30 W-BRN J2-13 LEFT SLINGSHOT**

**31 BRN-Y J2-14 POP BUMPER**

**32 -O- J2-15 LEFT LANE LOWER SWITCH**

**33 BRN J2-8 OUTHOLE**

**34 GREY J2-9 LEFT LANE KICK-OUT HOLE**

**35**  **W-O J2-10 ADVANCE SPINNER TO END**

**36 W-B J2-11 MIDDLE OUTHOLE SWITCH**

**37 W-G J2-12 LEFT OUTHOLE SWITCH**

**38 W-BRN J2-13 LEFT LANE MIDDLE SWITCH**

**39 BRN-Y J2-14 LEFT LANE TOP SWITCH**

**40 -O- J2-15 BALL SHOOTER LANE SWITCH**

**W-BLU (J2-3)**

**W-Y (J2-4)**

**Y-R (J2-5)**

Font used: Helvetica

Nine Ball Solenoid and Switch Identification card (size 248 x 187 mm) confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.