**STERN 16B-3 TRANSFORMER WIRING CONNECTION INSTRUCTIONS**

**220 / 240V., 50 / 60 Cycle Input.**

**Varistor - Soldered to Line Filter on Left Side of Cabinet.**

**Must be Stern Part No. 25A-18-2.**

**115 / 120V., 50 / 60 Cycle Input.**

**Varistor - Soldered to Line Filter on Left Side of Cabinet.**

**Must be Stern Part No. 25A-18-1.**

**Solder Heavy Red Wire  
To Lug 1**

**Solder Lugs 3 & 5  
Together**

**240V**

**Solder Heavy Yellow  
Wire To Lug 7**

**220V**

**Solder Heavy Yellow  
Wire To Lug 12**

**Solder Lugs 1 & 3  
Together. Solder Heavy  
Red Wire To Lug 1**

**120V**

**Solder Lugs 5 & 7  
Together. Solder Heavy  
Yellow Wire To Lug 5.**

**115V**

**Solder Lugs 9 & 11  
Together. Solder Heavy  
Yellow Wire To Lug 9**

1 3 5 7 9 11

2 4 6 8 10 12

1 3 5 7 9 11

2 4 6 8 10 12

**12A-153**

Font used: Helvetica, AlternateGothic2 BT, CentSchbook Mono BT

Size: 203 x 114 mm

12A-153 transformer card confirmed.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.