**NOTE:-**

B-432-FJ S.D.U. BOARD

FJ FLIPPER ENABLE RE. USES

ADDITIONAL JUMPER WIRES

TO INCREASE CURRENT

CAPABILITY.

12A-B-432-FJ

Fonts used: Arial Rounded MT Bold

Flipper Jumper label 12A-B-432-FJ confirmed (size 95x105mm).

If you have any more information, please send me a readable image.

Enjoy en have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.