##### Williams ***BANZAI RUN***

*OBJECT:* CHALLENGE and DEFEAT 4 riders to challenge the KING  
 OF THE HILL and become #1.

*CHALLENGE…* Riders by completing 3 of one color target on lower  
 playfield: Green, Yellow, Blue, Red.

*DEFEAT…* Any CHALLENGED rider by making matching color on  
 upper playfield.

*MULTI-BALL:* When all 4 opponents are DEFEATED, LOCK ball on  
 upper playfield to begin *Multi-Ball™.*

*BE #1……* in *Multi-Ball™*, LOCK 1 ball in Center Eject Hole; then use  
 other ball to defeat the KING OF THE HILL on upper play-  
 field to become #1.

*KICKBACK…* on left drain is lit by Center Eject Hole.

*LAPS……* around ramp increase lower Captive Ball value.

*SKILL SHOT…* from plunger challenges all 4 opponents.

16-566-1

##### Williams ***BANZAI RUN***

OBJET: DEFIER et BATTRE les 4 coureurs pour être LE ROI DE LA COLLINE  
 et devenir le No. 1.

CHALLENGE…Compléter 3 cibles de la même couleur sur le plateau inférieur:  
 Vert , Jaune , Bleu , Rouge.

BATTU (Defeat)…Chaque challenge est obtenu en faisant une couleur sur le plateau  
 supérieur.

MULTI-BILLE: Quand les 4 concurrents sont battus, verrouiller (Lock) une bille  
 sur le plateau supérieur pour commencer le jeu en Multi-Bille.

ETRE No. 1…En Multi-Bille, bloquer une bille dans l'éjecteur central, puis utiliser  
 l'autre bille pour battre LA ROI DE LA COLLINE en visant la 'bille  
 captive' sur le plateau supérieur.

RENVOI LATERAL (Kickback)…Sur le couloir de sortie gauche. Il s'allume par  
 l'entrée dans l'éjecteur central.

LAPS…passer sur la rampe augmente la valeur de la Bille Captive et enfin allume  
 l'Extra Bille.

POUR COUREURS EXPERTS SEULEMENT:

LIGNE D'ARRIVE (Finish Line)…Faites un maximum de tours (LAPS).

16-566-1-Fr

**WHEN MARQUEE IS  
RAISED UPRIGHT FOR ACCESSIBILITY, MARQUEE SUPPORT ARM MUST BE LOCKED IN ITS STRAIGHT POSITION.** 16-8587-939-2



**! WARNING**

**! WARNING**



**WHEN MARQUEE IS  
RAISED UPRIGHT FOR ACCESSIBILITY, MARQUEE SUPPORT ARM MUST BE LOCKED IN ITS STRAIGHT POSITION.** 16-8587-939-2

NEVER TRANSPORT A PINBALL GAME WITH THE HINGED BACKBOX ERECT.

*ALWAYS* LOWER THE BACKBOX FORWARD ONTO THE PLAYFIELD CABINET ON  
A LAYER OF PROTECTIVE MATERIAL TO PREVENT MARRING OR DAMAGE.

WHEN BACKBOX IS IN UPRIGHT POSITION, BACKBOX BOLTS ARE TO BE  
INSTALLED AT ALL TIMES.

FALURE TO DO THIS MAY RESULT IN POSSIBLE PERSONAL INJURY OR  
DAMAGE TO THE BACKBOX AND CABINET.

REFER TO SET-UP INSTRUCTIONS FOR PROPER ASSEMBLY OF BACKBOX.

16-8587-939-4

**! CAUTION**

INSTALL 3 BALLS (1 1/16 DIA) ON LOWER PLAYFIELD

INSTALL 1 BALL (15/16 DIA) IN FREESTYLE AREA

16-8587-939-9

MOTOR

TEST SWITCH

-939-1

MOTOR

TEST SWITCH

-939-1

REMOVE CAPTIVE BALL FROM FREESTYLE AREA BEFORE TRANSPORTING GAME 16-8587-939-6

REMOVE CAPTIVE BALL FROM FREESTYLE AREA BEFORE TRANSPORTING GAME 16-8587-939-6

! CAUTION DO NOT PIVOT PLAYFIELD WITH BALL CARRIER ALL THE WAY DOWN

16-8587-939-1

! CAUTION DO NOT PIVOT PLAYFIELD WITH BALL CARRIER ALL THE WAY DOWN

16-8587-939-1

! CAUTION THIS PIECE MUST BE REMOVED BEFORE LOWERING BACKBOX 16-8587-939-5

! CAUTION THIS PIECE MUST BE REMOVED BEFORE LOWERING BACKBOX 16-8587-939-5

**! CAUTION**

**! CAUTION**

**! CAUTION**

**! CAUTION**

Fonts used: New Venice, Times New Roman, HelveticaNeueLT Std Med, Helvetica.

**Cards status:**

16-566-1 confirmed.

16-566-1-Fr confirmed.

16-8587-939-1 needed to verify.

16-8587-939-2 warning label confirmed. (size: 80x127mm)

16-8587-939-3 needed.

16-8587-939-4 caution label confirmed, but I could use a good scan to adjust properly.

16-8587-939-5 caution label confirmed. (size: 323x10mm, but reduced to 250x10mm to fit the page better)

16-8587-939-6 confirmed.

16-8587-939-7 needed.

16-8587-939-8 needed.

16-8587-939-9 install balls label confirmed. (size: 133x19mm)

-939-1 Motor Test Switch label confirmed (size:12x38mm)

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.