• Liting any five bells in sequence, lites ONE red special spot.

• Liting any seven bells in sequence, lites TWO red special spots.

• Liting ten bells, lites THREE red special spots.

• Hole scores 1 REPLAY for each lited special spot.

• Matching last number in score to lited star that appears on back glass when game is over  
 scores 1 REPLAY.

###### 219-5A

5 BALLS 5 CENTS

###### GOLDEN BELLS

###### 5,500,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 1 Replay

###### 6,000,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 2 Replays

###### 7,000,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 3 Replays

###### 8,000,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 4 Replays

###### 8,500,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 5 Replays

For  
Amusement  
Only

Score Void  
If Game  
Is Tilted

###### GOLDEN BELLS

###### 5,500,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 1 Replay

###### 6,000,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 2 Replays

###### 7,000,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 3 Replays

###### 8,000,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 4 Replays

###### 8,500,000\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 5 Replays

• Liting any five bells in sequence, lites ONE red special spot.

• Liting any seven bells in sequence, lites TWO red special spots.

• Liting ten bells, lites THREE red special spots.

• Hole scores 1 REPLAY for each lited special spot.

• Matching last number in score to lited star that appears on back glass when game is over  
 scores 1 REPLAY.

###### 219-5A

5 BALLS 5 CENTS

For  
Amusement  
Only

Score Void  
If Game  
Is Tilted

No. 10

RELAY

X-30-1000

6 to 10

RELAY

X-30-1000

5 to 9

RELAY

X-30-1000

4 to 8

RELAY

X-30-1000

3 to 7

RELAY

X-30-1000

1 to 5

RELAY

X-30-1000

No. 9

RELAY

X-30-1000

2 to 6

RELAY

X-30-1000

###### G.B. 2

No. 2

RELAY

X-30-1000

No. 8

RELAY

X-30-1000

No. 7

RELAY

X-30-1000

No. 6

RELAY

X-30-1000

No. 5

RELAY

X-30-1000

No. 3

RELAY

X-30-1000

No. 1

RELAY

X-30-1000

No. 4

RELAY

X-30-1000

###### G.B. 2A

No. Match Cont.

RELAY

X-30-1000

5th BALL

RELAY

X-30-1000

GAME OVER

RELAY

X-30-1000

GAME

RELAY

X-30-1000

TILT

RELAY

X-30-1000

###### G.B. 2B

500,000

RELAY

Z-30-1800

50,000

RELAY

Z-30-1800

RESET

RELAY

Z-30-1800

START RELAY

LATCH TRIP

Z-30-1800 IT-35-4200

CHANGE

RELAY

Z-31-2300

ODD SPOT

RELAY

Z-30-1500

EVEN SPOT

RELAY

Z-30-1500

SPECIAL

RELAY

Z-30-1800

500,000

RELAY

Z-30-1800

###### G.B. 2C

LOCK

RELAY

Z-31-2300

CHANGE

RELAY

Z-31-2300

INSPECTION

Serial No.

1.

2.

3.

4.

5.

6.

7.

8.

9.

10.

FOR BACK DOOR KEY

STD. No. 13

INSERT BALLS HERE

STD. No. 68

**KICK-OFF SWITCH**

**Std. 65**

10,000 UNIT

STD. No. 1

100,000 UNIT

STD. No. 3

**TILT SWITCH**

**Std. 57**

MATCH UNIT

STD. No. 38

ADVISE LOCATION THAT TAPPING  
BOTTOM OF CABINET WILL TURN  
GAME OFF COMPLETELY.

**STD. 73**

**Special Adjustment Index  
Pos. Motor Sw.**

Motor run sw. wire colors  
Orange/Green and Yellow  
should make before 100,000  
reset cont. sw. wire colors  
Red/Blue and Green/White  
break.

**Std. 66**

**LITE BOX**

No 44874

**.**

**BACK DOOR**

No 44874

**.**

To replace light bulbs depress  
catch at top of cabinet and  
swing insert down.

VERY IMPORTANT

Be sure to insert all light box  
plugs BEFORE attaching cord  
to 110 V. line. Do not make  
any adjustments on contacts  
or step switches while ma-  
chine is connected to 110 V.  
line.

Std. 52

Fonts used: Futura Bk BT, Futura Hv BT, Futura Md BT, Times New Roman, Footlight MT, CentSchbook Mono BT

**Cards status:**

Card 219-5A confirmed.

Relay strips G.B. 2 & G.B. 2A are original two parts. I’ve made them into three parts to fit the paper.

SCS labels are available in a separate file called: SCS (coin/plays) inserts.

Balls per game cards are available in a separate file called: A.S.C. Balls per Game cards.

STD. No. 68 Insert Balls Here confirmed. This label is also known as STD. 54 (also confirmed).

STD. No. 13 For Back Door Key confirmed. This label is also known as STD. 12 (also confirmed).

STD-65 Kick-Off Switch confirmed. This label is also known as STD. 55 (also confirmed).

STD-57 Tilt Switch confirmed. This label is also known as STD. 52 (also confirmed).

Std. 66 Motor Switch label confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.