###### 3 OUTS PER INNING

###### 1 INNING PER PLAY

FOR  
AMUSEMENT  
ONLY

LINE DRIVE BASEBALL

###### 410-1

INNING  
VOID  
IF TILTED

###### 12 RUNS .................. 1 REPLAY

###### 18 RUNS .................. 1 REPLAY

###### 3 OUTS PER INNING

###### 2 INNINGS PER PLAY

FOR  
AMUSEMENT  
ONLY

LINE DRIVE BASEBALL

###### 410-2

INNING  
VOID  
IF TILTED

###### 14 RUNS .................. 1 REPLAY

###### 20 RUNS .................. 1 REPLAY

###### 3 OUTS PER INNING

###### 3 INNINGS PER PLAY

FOR  
AMUSEMENT  
ONLY

LINE DRIVE BASEBALL

###### 410-3

INNING  
VOID  
IF TILTED

###### 16 RUNS .................. 1 REPLAY

###### 22 RUNS .................. 1 REPLAY

INSTRUCTIONS

###### INSERT COIN TO START GAME

###### INSERT 2nd COIN FOR 2 PLAYERS

###### 410-5

###### BULLS EYE GRAND SLAM …….. 1 REPLAY

INSTRUCTIONS

###### INSERT COIN TO START GAME

###### INSERT 2nd COIN FOR 2 PLAYERS

###### 410-6

###### Bulls Eye Grand Slam ………. 1 Extra Inning

###### 14 RUNS .................. 1 REPLAY

###### 38 RUNS .................. 1 REPLAY

###### 410-xx

###### \_\_\_\_ RUNS ................. 1 REPLAY

###### \_\_\_\_ RUNS ................. 1 REPLAY

###### 410-xx

###### 14 RUNS ......... 1 EXTRA INNING

###### 38 RUNS ......... 1 EXTRA INNING

###### 410-12

###### \_\_\_\_ RUNS ......... 1 EXTRA INNING

###### \_\_\_\_ RUNS ......... 1 EXTRA INNING

###### 410-xx

###### 3rd GRAND SLAM ....... 1 REPLAY

###### 410-25

###### 3rd GRAND SLAM ....... 2 REPLAYS

###### 410-26

###### 3rd GRAND SLAM ....... 3 REPLAYS

###### 410-27

###### 6th GRAND SLAM ....... 1 REPLAY

###### 410-28

###### 6th GRAND SLAM ....... 2 REPLAYS

###### 410-29

###### 6th GRAND SLAM ....... 3 REPLAYS

###### 410-30

###### 9th GRAND SLAM ....... 3 REPLAYS

###### 410-33

###### 9th GRAND SLAM ....... 1 REPLAY

###### 410-31

###### 9th GRAND SLAM ....... 2 REPLAYS

###### 410-32

###### 3rd Grand Slam ....... 1 Extra Inning

###### 410-34

###### 3rd Grand Slam ...... 2 Extra Innings

###### 410-35

###### 3rd Grand Slam ...... 3 Extra Innings

###### 410-36

###### 6th Grand Slam ....... 1 Extra Inning

###### 410-37

###### 6th Grand Slam ...... 2 Extra Innings

###### 410-38

###### 6th Grand Slam ...... 3 Extra Innings

###### 410-39

###### 9th Grand Slam ...... 3 Extra Innings

###### 410-42

###### 9th Grand Slam ....... 1 Extra Inning

###### 410-40

###### 9th Grand Slam ...... 2 Extra Innings

###### 410-41

###### 423-6

###### NORMAL

###### CONSERVATIVE

###### NORMAL- CONSERV. ADJUSTMENT

###### INNING ADJUSTMENT

###### 1

###### 2

###### 3

###### 423-11

###### CREDIT

###### ADJUSTMENT

###### EXTRA INNING

###### 423-7

###### GRAND SLAM ADJUSTMENT

###### 3 6 9

###### 423-8

###### 3 RD OUT RELAY

###### Z-27-1000

###### 423-10

###### BLU-W GRAND SLAM

###### B-O HI-SCORE ADJ.

###### 423-12

###### 423-9

###### 1 2 3

###### GRAND SLAM SCORE ADJUSTMENT

###### HOME RUN RELAY M-30-1400

###### NO. 1 RELAY M-29-1100

###### NO. 2 RELAY M-29-1100

###### NO. 3 RELAY M-29-1100

###### Attach to the next strip at the dotted line.

###### NO. 4 RELAY M-29-1100

###### GRAND SLAM RELAY M-30-1400

###### 423-1

###### OUT RELAY M-29-1100

###### Attach to the next strip at the dotted line.

###### LOCK RELAY Z-28-1200

###### LOAD RELAY Z-28-1150

###### TILT RELAY Z-28-1150

###### COIN RELAY Z-28-1000

###### START RELAY Z-27-1000

###### SWING RELAY Z-28-1150

###### 423-2

###### BAT RELAY Z-28-1150

###### PITCH RELAY Z-28-1150

###### STRIKE RELAY M-30-1400

###### 423-3

###### BAT BUTTON RELAY M-29-1100

1 2

PLAY PLAYS

10c

COIN ADJ.

STD. 79

###### SLAM SWITCH CONTACTS NORMALLY CLOSED

STD. 400

**25**¢

**ADJ.**

5

4

3

2

STD. 446

NOTICE

THIS GAME OPERATES

ON **24 VOLTS**

###### STD. 8A

MOTOR-SERVICE JACK

ON OFF

**STD. 99**

BAT UNIT

END OF STROKE  
SWITCH OPENS  
CIRCUIT TO BAT  
RELAY.

STD. 428

HI-SCORE ADJUSTMENT

PLUG IN RED  
WIRE FOR SCORES  
11 TO 20

PLUG IN BLUE  
WIRE FOR SCORES  
21 TO 30

PLUG IN YELLOW  
WIRE FOR SCORES  
31 TO 40

PLUG IN GREEN  
WIRE FOR SCORES  
41 TO 50

EXAMPLE :

BLUE WIRE INTO 1 POSITION SCORES AT 21 OR  
BLUE WIRE INTO 0 POSITION SCORES AT 30.

400-6

POINT SCORE STORAGE  
ADJUSTMENT AREA

1

2

3

4

5

6

7

8

9

0

###### DECREASE INCREASE

###### BAT POWER

###### CONTROL

###### 370-12

TO REMOVE PLAYFIELD

**LOOSEN (2) WING NUTS, THEN TURN HOLDING BRACKET IN.**

423-13

LINE DRIVE SOUND UNIT- 20A-9038

WE 1020

UA10

FUSE ¼ AMP

5A-8745

GM123

GM108

GM110

SIREN

CROWD

EXPLOSION

AMPLIFIER

16C-423-5

Fonts used: Alternate Gothic No.2, Helvetica Inserat LT Std, HelveticaNeue, Helvetica LT Std, Futura Md BT,   
Century, Futura Hv BT, Helvetica 55 Roman, News Gothic Demi

Card sizes: score cards 95x54mm, score inserts 95x24mm, instruction cards 95x54mm, insert strips 95x17mm

**Cards status:**

All card, inserts and labels confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.