**NOTICE**

TO CONVERT TO 115 VOLT OPERATION, REMOVE LINE CORD WIRE FROM 230 VOLT TAP AND SOLDER TO 115 VOLT TAP.

TO CONVERT TO 230 VOLT OPERATION, REMOVE LINE CORD WIRE FROM 115 VOLT TAP AND SOLDER TO 230 VOLT TAP.

**STD. 13A**

Fonts used: Futura Hv BT, Century

Size: 178x50mm

STD-13A Notice (voltage adjustment).

If you have more labels like this, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.